Xircom Ethernet 10/100+Modem 56 - Specifications

#

Table of Contents | Previous Page | Next Page

# Ethernet 10/100+Modem 56
Specifications

- General Specifications by Model
- Modem Specifications

## General Specifications by Model

###

| Xircom RealPort Ethernet 10/100+Modem 56 (REM56G-100)
PC Card Type | Type III PC Card
Connectors | RJ-45 (for 100Base-TX/10Base-T Ethernet), RJ-11 (modem), RJ-11 (phone set pass-through), mini D-Sub for GSM, PDC, ISDN (separate connection kit required)
Size | 86.0 mm x 54.0 mm x 10.5 mm (3.37 x 2.13 x 0.413 inches)
Weight | 36 g (1.3 oz)

Ethernet | IEEE 802.3 10Mbps, full- and half-duplex
| IEEE 802.3u 100Mbps, full- and half-duplex
Ethernet Cables |
100Base-TX | Unshielded twisted pair (UTP) Category 5 (data grade)
10Base-T | Unshielded twisted pair (UTP)
Temperature range |
Operating | 32°F to 149°F (0°C to 65°C)
Storage | -4°F to 185°F (-20°C to 85°C)
Humidity | 95% maximum no condensing
Memory | 4 megabits memory for dual V.90 and K56flex
Power Requirements |
10Base-T | 3.3V DC, 80 mA idle, 100 mA active
100Base-TX | 3.3V DC, 130 mA idle, 160 mA active
Modem only | 3.3V DC, 40 mA sleep, 240 mA active
10Base-T+Modem | 3.3V DC, 250 mA idle, 265 mA active
100Base-TX+Modem | 3.3V DC, 260 mA idle, 340 mA active
BatterySaveTM (LAN cable disconnected) | 45 mA
Approvals | FCC Part 15, Part 68, Industry Canada, CE Mark

##

| Xircom CreditCard Ethernet 10/100+Modem 56 (CEM56-100)
PC Card Type | Type II PC Card
Connectors | RJ-45 (for 100Base-TX/10Base-T Ethernet), BNC (10Base-2 Ethernet), RJ-11 (modem), GSM/PDC/ISDN/PCS 1900/cellular (via optional connection kit)
Size | 86.0 mm x 54.0 mm x 5 mm (3.37 x 2.13 x 0.197 inches)
Weight | 42.1 g (1.47 oz)

Ethernet | IEEE 802.3 10Mbps, full- and half-duplex
| IEEE 802.3u 100Mbps, full- and half-duplex
Ethernet Cables |
100Base-TX | Unshielded twisted pair (UTP) Category 5 (data grade)
10Base-T | Unshielded twisted pair (UTP)
10Base-2 | BNC
Temperature range |
Operating | 32°F to 131°F (0°C to 55°C)
Storage | -4°F to 149°F (-20°C to 65°C)
Humidity | 95% maximum noncondensing
Memory | 4 megabits memory for dual V.90 and K56flex
Power Requirements | +5 VDC, 490 mA typical
BatterySaveTM (LAN cable disconnected) | 45 mA
Approvals | FCC Part 15, Part 68, Industry Canada, CE Mark

## Modem Specifications

Data modulation | V.90/K56flex up to 56000 bps; V.34 from 33,600 down to 2400 bps; V.32terbo at 19200 and 16800 bps; V.32bis at 14400, 12000, 9600, and 7200 bps, uncoded at 4800 bps; V.32 at 9600 bps, uncoded at 4800 bps; V.23 at 1200/75 and 75/1200 bps; V.22bis at 2400 bps; V.22 at 1200 bps; Bell 212A at 1200 bps
Fax modulation | V.17 at 14400, 12000, 9600, 7200, and 4800 bps; V.29 at 9600, 7200, and 4800 bps; V.27ter at 4800 and 2400 bps
Fax support | Group 3, EIA/TIA Class 1
Error control | V.42 Error Control, MNP Levels 2-4 Error Detection
Data compression | V.42bis (4:1) or MNP Level 5 (2:1)
Diagnostics: | Power-up self tests of program RAM, data RAM, and nonvolatile memory
Nonvolatile RAM | 1 user definable profile; 2 thirty-six digit telephone numbers; LAN Adapter ID and serial number
Command set | Hayes and Microcom compatible AT commands
Data interface | PCMCIA Release 2.1 compliant, 68-pin connector
Analog interface | RJ-11C modular telephone connector
DTE speeds | 1200, 2400, 4800, 7200, 9600, 14400, 19200, 37400, 57600, and 115200 bps

Table of Contents | Previous Page | Next Page