InS_StArT
XCEMODI.COM
1.1
^Xircom Ethernet 10/100 Adapter,XCEMODI.COM,IEM
?The Xircom Ethernet 10/100 Adapter runs on laptops equipped with a PCMCIA socket. All parameters default to automatic detection or selection if left blank.
*RIEM000(FRAME)Media Frame Type(s)
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$OIEM000(IRQ)Adapter IRQ
?This parameter is used to set the LAN interrupt. Leave this parameter blank for automatic detection.
3
15
$OIEM000(MEMORY)Adapter Memory Address
?The adapter uses a 4 kbyte window aligned on 4 kbyte boundaries (D2000, D3000, etc). Leave this parameter blank for automatic detection.
C0000
EF000
$OIEM000(IOADDRESS)Adapter I/O Address
?The adapter uses 32 I/O locations aligned on a 32 byte boundary (100, 120, etc.). Using this parameter will force the adapter to use I/O mode instead of memory mode. Leave this parameter blank for automatic detection.
100
FF80
$OIEM000(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
$OIEM000(SOCKET)PCMCIA Socket
?Use this parameter to force the driver to use a particular socket. Leave this parameter blank for automatic detection.
1
4
$OIEM000(TXBUFFERSIZE)Transmit buffer size (in packets)
?Set the size of the adapter's transmit packet buffer in decimal. Leave this parameter blank for the default size (2).
1
20
!OIEM000(LINESPEED)Line speed
?Select either 10 Mbits/sec or 100 Mbits/sec. Make sure your network cabling supports the speed you select. Leave this parameter blank for automatic detection (auto-negotiation).
10
100
!OIEM000(LINEMODE)Line mode
?Select half-duplex or full-duplex mode. Your network hardware must support full-duplex if you select FULL. Leave this parameter blank for automatic detection (auto-negotiation).
HALF
FULL
InS_EnD
