;******************************************************************************
;
; OEMSETNT.INF 
;
;       Xircom Ethernet 10/100 + Modem 56 Network Adapter Setup
;
;  $Revision:   1.30  $
;
;	with Resource Detect, NDIS Switch, Softex merge 06/12/2000
;
;-------------------------------------------------------------------------
;	if (Softex)
;		{CEM56NT.SYS}
;
;	else (STANDARD NT4)
;		{CEM56N4.SYS, CEM56.SYS, MODEM.IN_, Ndis Switch}
;-------------------------------------------------------------------------
;
;******************************************************************************

[Identification]
    OptionType = NetAdapter

[PlatformsSupported]
    ISA
    EISA
    MCA

[Options]
	CEM56

[OptionsTextENG]
    CEM56    = "Xircom Ethernet 10/100+Modem 56"

;;;-----START---AllFileConstantsSoftex----------;;;
[AllFileConstantsSoftex]
GenericInfVersion  = " v2.56"
;  File names, etc. ----------------------------------------
UtilityInf      = "UTILITY.INF"
ParamInf        = "NCPARAM.INF"
subroutineinf   = "SUBROUTN.INF"
SoftwareType    = "driver"
Exit_Code       = 0
; EventLog Message File	 ----------------------------------------
NetEventDLL     = "%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\drivers\cem56nt.sys"
IoLogMsgDLL     = "%SystemRoot%\System32\IoLogMsg.dll"
; Product Info ----------------------------------------
Manufacturer    = "Xircom"
; Flow control variables  ----------------------------------------
RUNDLLCODE	 = 1
;HOTPROGRAMPCMCIA = 1

GenericTextName = "Ethernet 10/100+Modem 56 for Softex"
DEFAULT_LANMEM = 1		;Auto
DEFAULT_LANIO = 1		;Auto
DEFAULT_IRQ = 1			;Auto
DEFAULT_MODEMIO = 1		;Auto
DEFAULT_COM  = 2		; COM2
;;;-----END---AllFileConstantsSoftex----------;;;

;;;-----START---AllFileConstants----------;;;
[AllFileConstants]
GenericInfVersion  = " v2.56"
;  File names, etc. ----------------------------------------
UtilityInf      = "UTILITY.INF"
ParamInf        = "NCPARAM.INF"
subroutineinf   = "SUBROUTN.INF"
SoftwareType    = "driver"
Exit_Code       = 0
; EventLog Message File	 ----------------------------------------
NetEventDLL     = "%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\drivers\CEM56N4.sys"
IoLogMsgDLL     = "%SystemRoot%\System32\IoLogMsg.dll"
; Product Info ----------------------------------------
Manufacturer    = "Xircom"
; Flow control variables  ----------------------------------------
RUNDLLCODE	 = 1
HOTPROGRAMPCMCIA = 1
;;;-----END---AllFileConstants----------;;;

;;;-----START---FileConstantsSoftex-CEM56----------;;;
[FileConstantsSoftex-CEM56]
GenericAdapterName = "Xircom Ethernet 10/100+Modem 56 for Softex"
GenericDriverName  = "Xircom Ethernet 10/100+Modem 56 for Softex"
GenericSysName     = "CEM56NT.sys"
GenericName        = "CEM56NT"
; Product Info ----------------------------------------
ProductMajorVersion     = "3"
ProductMinorVersion     = "12"
ProductVersion  = $(ProductMajorVersion)"."$(ProductMinorVersion)
; Software  ----------------------------------------
ProductSoftwareName     = "CEM56NT"
ProductSoftwareDescription = "Xircom Ethernet 10/100+Modem 56"
ProductSoftwareImagePath = "\SystemRoot\System32\drivers\"$(GenericSysName)
NetRuleSoftwareType     = "cem56ntSys ndisDriver cem56ntDriver"
NetRuleSoftwareUse      = $(SoftwareType)
NetRuleSoftwareBindForm = """cem56ntSys"" yes no container"
NetRuleSoftwareClass    = {"cem56ntDriver basic"}
NetRuleSoftwareBindable = {"cem56ntDriver cem56ntAdapter non exclusive 100"}
; Hardware  ----------------------------------------
ProductHardwareName        = "CEM56NT"
ProductHardwareDescription = "Xircom Ethernet 10/100+Modem 56 for Softex"
NetRuleHardwareType        = "cem56nt cem56ntAdapter"
NetRuleHardwareBindForm    = " yes yes container"
NetRuleHardwareClass       = {"cem56ntAdapter basic"}
; Registry Key  ----------------------------------------
ProductKeyName  = $(!NTN_SoftwareBase)"\"$(Manufacturer)"\"$(ProductSoftwareName)"\CurrentVersion"
ParamKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)"\Parameters"
; Tuple Information -----------------------------------
VERS1Manufacturer = "Xircom"
VERS1Product      = "CreditCard Ethernet 10/100 + Modem 56 for Softex"
;;;-----END---FileConstantsSoftex-CEM56----------;;;

;;;-----START---FileConstants-CEM56----------;;;
[FileConstants-CEM56]
GenericAdapterName = "Xircom Ethernet 10/100+Modem 56"
GenericDriverName  = "Xircom Ethernet 10/100+Modem 56"
GenericSysName     = "CEM56N4.sys"
GenericName        = "CEM56"
; Product Info ----------------------------------------
ProductMajorVersion     = "3"
ProductMinorVersion     = "12"
ProductVersion  = $(ProductMajorVersion)"."$(ProductMinorVersion)
; Software  ----------------------------------------
ProductSoftwareName     = "CEM56"
ProductSoftwareDescription = "Xircom Ethernet 10/100+Modem 56"
ProductSoftwareImagePath = "\SystemRoot\System32\drivers\"$(GenericSysName)
NetRuleSoftwareType     = "cem56Sys ndisDriver cem56Driver"
NetRuleSoftwareUse      = $(SoftwareType)
NetRuleSoftwareBindForm = """cem56Sys"" yes no container"
NetRuleSoftwareClass    = {"cem56Driver basic"}
NetRuleSoftwareBindable = {"cem56Driver cem56Adapter non exclusive 100"}
; Hardware  ----------------------------------------
ProductHardwareName        = "CEM56"
ProductHardwareDescription = "Xircom Ethernet 10/100+Modem 56"
NetRuleHardwareType        = "cem56 cem56Adapter"
NetRuleHardwareBindForm    = " yes yes container"
NetRuleHardwareClass       = {"cem56Adapter basic"}
; Registry Key  ----------------------------------------
ProductKeyName  = $(!NTN_SoftwareBase)"\"$(Manufacturer)"\"$(ProductSoftwareName)"\CurrentVersion"
ParamKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)"\Parameters"
; Tuple Information -----------------------------------
VERS1Manufacturer = "Xircom"
VERS1Product      = "CreditCard Ethernet 10/100 + Modem 56"
;;;-----END---FileConstants-CEM56----------;;;


[GeneralConstants]
;  Program flow control variables.
from      = ""
to        = ""
;  Return codes; Exit_Code is set to one of these
ExitCodeOk     = 0
ExitCodeCancel = 1
ExitCodeFatal  = 2
KeyNull         = ""
MAXIMUM_ALLOWED   = 33554432
RegistryErrorIndex = NO_ERROR
KeyProduct      = ""
KeyParameters   = ""
TRUE            = 1
FALSE           = 0
NoTitle            = 0
ExitState   = "Active"
OldVersionExisted = $(FALSE)
DriverPath      = $(!STF_NTPATH)\drivers
;BCM




[date]
    ; Now is a list which contains { Sec from 1-1-1970, Year, Month, Day, Hour,
    ; Minute, Second }
    Now = {} ? $(!LIBHANDLE) GetSystemDate


;---------------------------------------------------------------------------
; 1. Identify
;
; DESCRIPTION:   To verify that this INF deals with the same type of options
;                as we are choosing currently.
;
; INPUT:         None
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL
;                $($R1): Option Type (COMPUTER ...)
;                $($R2): Diskette description
;---------------------------------------------------------------------------

[Identify]
    ;
    ;
    read-syms Identification

    set Status     = STATUS_SUCCESSFUL
    set Identifier = $(OptionType)
    set Media      = #("Source Media Descriptions", 1, 1)

    Return $(Status) $(Identifier) $(Media)

;------------------------------------------------------------------------
; 2. ReturnOptions:
;
; DESCRIPTION:   To return the option list supported by this INF and the
;                localised text list representing the options.
;
;
; INPUT:         $($0):  Language used. ( ENG | FRN | ... )
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL |
;                                STATUS_NOLANGUAGE
;                                STATUS_FAILED
;                                STATUS_NOTSUPPORTED
;
;                $($R1): Option List
;                $($R2): Option Text List
;------------------------------------------------------------------------

[ReturnOptions]
    ;
    ;
    set Status        = STATUS_FAILED
    set OptionList     = {}
    set OptionTextList = {}

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) in $(LanguageList)
        ;
        ; Check if the platforms requested is supported
        ;
        ifstr(i) $($1) == ""
                        goto returnoptions
        endif

        set PlatformList = ^(PlatformsSupported, 1)
        Ifcontains(i) $($1) in $(PlatformList)
                        goto returnoptions
        else
                        set Status = STATUS_NOTSUPPORTED
                        goto finish_ReturnOptions
        endif
    else
                set Status = STATUS_NOLANGUAGE
                goto finish_ReturnOptions
    endif

    ;
    ; form a list of all the options and another of the text representing
    ;

returnoptions = +
    set OptionList     = ^(Options, 1)
    set OptionTextList = ^(OptionsText$($0), 1)
    set Status         = STATUS_SUCCESSFUL

finish_ReturnOptions = +
    Return $(Status) $(OptionList) $(OptionTextList)

;------------------------------------------------------------------------
;
; InstallOption:
;
;      This section is shelled to by main installation processing
;      or by NCPASHEL.INF during reconfig, removal, update, etc.
;
;
; FUNCTION:  To copy files representing Options
;            To configure the installed option
;            To update the registry for the installed option
;
; INPUT:     $($0):  Language to use
;            $($1):  OptionID to install
;            $($2):  SourceDirectory
;            $($3):  AddCopy  (YES | NO)
;            $($4):  DoCopy   (YES | NO)
;            $($5):  DoConfig (YES | NO)
;
; OUTPUT:    $($R0): STATUS: STATUS_SUCCESSFUL |
;                            STATUS_NOLANGUAGE |
;                            STATUS_USERCANCEL |
;                            STATUS_FAILED
;
;------------------------------------------------------------------------
[InstallOption]
    ;
    ; Set default values for
    ;
    set Status   = STATUS_FAILED
    ;
    ; extract parameters
    ;
    set Option   = $($1)
    set SrcDir   = $($2)
    set AddCopy  = $($3)
    set DoCopy   = $($4)
    set DoConfig = $($5)

    Set !DebugOutputControl = 1

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) NOT-IN $(LanguageList)
        Return STATUS_NOLANGUAGE
    endif

    set-subst LF = "\n"

	;--------------------------------------
	;;;start Resource Detect

	set CSInstalled = "STANDARD NT4"

	ifstr(i) $(!NTN_InstallMode) == "install"
		LoadLibrary "disk1" $(SrcDir)"CEM56.DLL" hLib
	else
		LoadLibrary "disk1" $(!STF_WINDOWSSYSPATH)"\CEM56.DLL" hLib
	endif

	LibraryProcedure CSInstalled, $(hLib), IsSoftex

    read-syms GeneralConstants
	
	ifstr(i) $(CSInstalled) == "Softex"

		read-syms AllFileConstantsSoftex
		read-syms FileConstantsSoftex"-"$(Option)

    else-ifstr(i) $(CSInstalled) == "STANDARD NT4"

		read-syms AllFileConstants
		read-syms FileConstants"-"$(Option)

	endif

	read-syms DialogConstants$(!STF_LANGUAGE)"-"$(Option)

	ifstr(i) $(!NTN_Origination) == "NCPA"
        set Continue = $(OK)
    endif

    read-syms AllFileConstants$(!STF_LANGUAGE)

	ifstr(i) $(CSInstalled) == "Softex"	

		read-syms FileConstantsSoftex$(!STF_LANGUAGE)"-"$(Option)

	else-ifstr(i) $(CSInstalled) == "STANDARD NT4"

		read-syms FileConstants$(!STF_LANGUAGE)"-"$(Option)

	endif

    detect date

    set-title  $(FunctionTitle)

    set to   = Begin
    set from = Begin
;
;  Assume all is well.
;
    set CommonStatus = STATUS_SUCCESSFUL

    EndWait

;
;   Set up the operation-mode-based variables and gaily welcome
;   the user.  If the "install mode" variable is improperly set,
;   assume this is a new installation.
;

Begin = +
    Set ActivateDetection = FALSE

    Ifstr(i) $(!NTN_InstallMode) == deinstall
        set StartLabel = removeadapter
    else-Ifstr(i) $(!NTN_InstallMode) == Update
        set StartLabel = UpgradeSoftware
    else-Ifstr(i) $(!NTN_InstallMode) == bind
        set StartLabel = bindingadapter
    else-Ifstr(i) $(!NTN_InstallMode) == configure
;        set ActivateDetection = TRUE
        set StartLabel = configureadapter
        ;
        ;   You cannot config the software component
        ;
        Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
            ;Debug-Output "Cannot configure the software."
            Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_SOFTWARE
            ifint $($ShellCode) != $(!SHELL_CODE_OK)
                Debug-Output "ShellCode error: cannot get an error string."
                goto ShellCodeError
            endif
            set Error = $($R0)
            set from = end
            set to = end
            goto nonfatalinfo
        endif
    else
;        set ActivateDetection = TRUE
        set StartLabel = installadapter
        set OEM_ABANDON_OPTIONS = {}
        set OEM_ABANDON_SOFTWARE = FALSE
        set OEM_ABANDON_ON = TRUE
    endif


	;  set the [Default values]
	ifstr(i) $(CSInstalled) == "Softex"

		set IRQValue			= *($(IRQList), $(DEFAULT_IRQ))	; IRQ Level      
		set IOBaseAddrValue		= *($(IOBaseAddrList), $(DEFAULT_LANIO)) ; IOBase 
		set MemoryAddrValue		= *($(MemoryAddrList), $(DEFAULT_LANMEM)) ; Memory 
		set ComIOBaseAddressValue	= *($(ComIOBaseAddressList), $(DEFAULT_MDMIO))	; ComIOBase 
		set COMStringValue		= *($(COMStringList), $(DEFAULT_COM)) ; May AutoDetect this later! 
		set EarlyTransmitValue		= "ON"				; Early Transmit = on
		set LinkIntegrityValue		= "ON"				; Link Integrity = Enabled
		set DynamicLinkDetectValue	= "ON"				; Dynamic Link Detection = on
		set ModeValue			= *($(ModeList), 1)		; Mode           = I/O
		set LineSpeedValue		= *($(LineSpeedList), 1)	; LineSpeed      = auto
		set LineModeValue		= *($(LineModeList), 1)		; LineMode       = auto
		set InitDelayValue		= *($(InitDelayList), 1)	; InitDelay = 0
	
	else-ifstr(i) $(CSInstalled) == "STANDARD NT4"

		set IRQValue			= *($(IRQList), 8)		; IRQ Level      = 11
		set IOBaseAddrValue		= *($(IOBaseAddrList), 18)	; IOBase Address = 0x320
		set MemoryAddrValue		= *($(MemoryAddrList), 53)	; Memory Address = 0xD0000
		set ComIOBaseAddressValue	= *($(ComIOBaseAddressList), 4)	; ComIOBase Address = 2e8(COM4)
		set EarlyTransmitValue		= "ON"				; Early Transmit = on
		set LinkIntegrityValue		= "ON"				; Link Integrity = Enabled     
		set DynamicLinkDetectValue	= "ON"				; Dynamic Link Detection = on
		set ModeValue			= *($(ModeList), 1)		; Mode           = I/O
		set LineSpeedValue		= *($(LineSpeedList), 1)	; LineSpeed      = auto
		set LineModeValue		= *($(LineModeList), 1)		; LineMode       = auto
		set FEnableValue		= *($(FEnableList), 1)		; FEnable        = Network & Modem
		set InitDelayValue		= *($(InitDelayList), 1)        ; InitDelay = 0
		set NdisVersionValue	= *($(NdisVersionList), 1)					; NdisVersion = 4
		
	endif

    Set from = $(fatal)
    Set to = $(fatal)
    Goto $(StartLabel)

;-----------------------------------------------
; Installation Section
;-----------------------------------------------

installadapter = +
;
;   First, check whether the same version of the software exists
;
    OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

    Ifstr $(KeyProduct) != $(KeyNull)
        ;
        ; Same version already existed in the local machine
        ; Popup the dialog and ask the user whether he wants to continue
        ;
        CloseRegKey $(KeyProduct)

        ifstr(i) !(NTN_RegBase) == $(ProductKeyName)
           ;
           ; Cannot Install the same software again
           ;
           Shell $(UtilityInf), VerExistedDlg, $(ProductSoftwareTitle),+
               $(ProductVersion)
           ifint $($ShellCode) != $(!SHELL_CODE_OK)
               Debug-Output "ShellCode error: cannot get an error string."
               goto ShellCodeError
           endif

           goto end
        else
           ;
           ; Add a new adapter card?
           ;
           Shell $(UtilityInf), CardExistedDlg

           ifint $($ShellCode) != $(!SHELL_CODE_OK)
               Debug-Output "ShellCode error: cannot get an error string."
               goto ShellCodeError
           endif

           ifstr(i) $($R1) != "OK"
               goto end
           endif
           set OldVersionExisted = $(TRUE)
        endif
    endif

;
;  dll load addition
;
    Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) NO

    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Goto ShellCodeError
    Else-Ifstr(i) $($R0) == STATUS_FAILED
        Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
        Goto fatal
    Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
        Goto successful
    Endif

    Set SrcDir = $($R1)

    install "Install-Dll"

    goto adaptersetup

;-----------------------------------------------
; Configuration Section
;-----------------------------------------------
;
;   Get the current values of all the parameters
;
configureadapter = +
    Ifstr $(KeyProduct) == $(KeyNull)
        OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) $(MAXIMUM_ALLOWED) KeyProduct
        Ifstr $(KeyProduct) == $(KeyNull)
            set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
            Debug-Output "Cannot find component product key"
            goto fatalregistry
        Endif
    Endif

    ;
    ; Get the other parameters;  they're attached to the service parameters key
    ;
    Debug-Output "INF: Shelling to FindService"
    Shell $(UtilityInf) FindService, $(KeyProduct)
    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "INF: FindService shell failure"
        Goto ShellCodeError
    Endif
    Ifstr(i) $($R0) != NO_ERROR
        Debug-Output "INF: FindService Shell error: "$($R0)
        Goto fatalregistry
    endif

    Set KeyParameters = $($R2)

    ;
    ;  We don't need the services key, so close it.
    ;
    CloseRegKey $($R1)

    Ifstr $(KeyParameters) == $(KeyNull)
        set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
        Debug-Output "Cannot find component service"
        goto fatalregistry
    endif

    set OldVersionExisted = $(TRUE)

    set ValueName = ""
    set ValueData = ""
    set ValueStr  = ""
    set ValueList = {}

	
    ;
    ; Get the old values from the Registry	[Get Values]
    ; *********************************************************
	EnumRegValue $(KeyParameters) ValueList
    ForListDo $(ValueList)
		set ValueItem = $($)
		set ValueName = *($(ValueItem),1)
		set ValueData = *($(ValueItem),4)
		ifstr(i) $(ValueName) == "IoBaseAddress_1"
		    set IOBaseAddrIndex = $(ValueData)
		else-ifstr(i) $(ValueName) == "InterruptNumber"
		    set IRQValueIndex = $(ValueData)
		else-ifstr(i) $(ValueName) == "EarlyTransmit"
		    set EarlyTransmitValue = $(ValueData)
		else-ifstr(i) $(ValueName) == "LinkIntegrity"
		    set LinkIntegrityValue = $(ValueData)
		else-ifstr(i) $(ValueName) == "DynamicLinkDetect"
		    set DynamicLinkDetectValue = $(ValueData)
		else-ifstr(i) $(ValueName) == "IoBaseAddress"
		    set ComIOBaseAddressIndex = $(ValueData)
		else-ifstr(i) $(ValueName) == "PCCARDAttributeMemoryAddress"
		    set MemoryAddrIndex = $(ValueData)
		else-ifstr(i) $(ValueName) == "NetworkAddress"
		    set NetworkAddressValue = $(ValueData)
		else-ifstr(i) $(ValueName) == "Mode"
		    set ModeIndex = $(ValueData)                ; mode value is base 0
		else-ifstr(i) $(ValueName) == "LineSpeed"
		    set LineSpeedIndex = $(ValueData)                
		else-ifstr(i) $(ValueName) == "LineMode"
		    set LineModeIndex = $(ValueData)                

		else-ifstr(i) $(ValueName) == "FunctionEnable"
		    set FEnableIndex = $(ValueData)

		else-ifstr(i) $(ValueName) == "ComNumber"
		    set COMStringIndex = $(ValueData)    

		else-ifstr(i) $(ValueName) == "InitDelay"
		    set InitDelayIndex = $(ValueData)  
		
		else-ifstr(i) $(ValueName) == "NdisVersion"
			set NdisVersionIndex = $(ValueData)
		endif
    EndForListDo

	ifstr(i) $(CSInstalled) == "Softex"

		set COMStringValue = *($(COMStringList), ~($(COMStringValues),$(COMStringIndex)))
		ifstr(i) $(COMStringValue) == ""
		set COMStringValue = *($(COMStringList), $(DEFAULT_COM))
		endif

		set IRQValue = *($(IRQList), ~($(IRQValues),$(IRQValueIndex)))
		ifstr(i) $(IRQValue) == ""
		set IRQValue = *($(IRQList), $(DEFAULT_IRQ))
		endif

		set MemoryAddrValue = *($(MemoryAddrList), ~($(MemoryAddrValues),$(MemoryAddrIndex)))
		ifstr(i) $(MemoryAddrValue) == ""
		set MemoryAddrValue = *($(MemoryAddrValues), $(DEFAULT_LANMEM))
		endif

		set IOBaseAddrValue = *($(IOBaseAddrList), ~($(IOBaseAddrValues),$(IOBaseAddrIndex)))
		ifstr(i) $(IOBaseAddrValue) == ""
		set IOBaseAddrValue = *($(IOBaseAddrList), $(DEFAULT_LANIO))
		endif

		set ComIOBaseAddressValue = *($(ComIOBaseAddressList), ~($(ComIOBaseAddressValues),$(ComIOBaseAddressIndex)))
		ifstr(i) $(ComIOBaseAddressValue) == ""
		set ComIOBaseAddressValue = *($(ComIOBaseAddressValues), $(DEFAULT_MDMIO))
		endif

	else-ifstr(i) $(CSInstalled) == "STANDARD NT4"
    
		set IRQValue = *($(IRQList), ~($(IRQValues),$(IRQValueIndex)))
		ifstr(i) $(IRQValue) == ""
		set IRQValue = *($(IRQList), 2)
		endif

		set MemoryAddrValue = *($(MemoryAddrList), ~($(MemoryAddrValues),$(MemoryAddrIndex)))
		ifstr(i) $(MemoryAddrValue) == ""
		set MemoryAddrValue = *($(MemoryAddrValues), 2)
		endif

		set IOBaseAddrValue = *($(IOBaseAddrList), ~($(IOBaseAddrValues),$(IOBaseAddrIndex)))
		ifstr(i) $(IOBaseAddrValue) == ""
		set IOBaseAddrValue = *($(IOBaseAddrList), 1)
		endif

		set ComIOBaseAddressValue = *($(ComIOBaseAddressList), ~($(ComIOBaseAddressValues),$(ComIOBaseAddressIndex)))
		ifstr(i) $(ComIOBaseAddressValue) == ""
		set ComIOBaseAddressValue = *($(ComIOBaseAddressValues), 2)
		endif
	
		set NdisVersionValue = *($(NdisVersionList), ~($(NdisVersionValues),$(NdisVersionIndex)))
		ifstr(i) $(NdisVersionValue) == ""
			set NdisVersionValue = *($(NdisVersionValues), 1)
		endif
	
	endif

    set ModeValue = *($(ModeList), ~($(ModeValues),$(ModeIndex)))
    ifstr(i) $(ModeValue) == ""
	set ModeValue = *($(ModeValues), 2)
    endif

    set LineSpeedValue = *($(LineSpeedList), ~($(LineSpeedValues),$(LineSpeedIndex)))
    ifstr(i) $(LineSpeedValue) == ""
	set LineSpeedValue = *($(LineSpeedValues), 0)
    endif

    set LineModeValue = *($(LineModeList), ~($(LineModeValues),$(LineModeIndex)))
    ifstr(i) $(LineModeValue) == ""
	set LineModeValue = *($(LineModeValues), 0)
    endif

    ifstr(i) $(CSInstalled) == "STANDARD NT4"
		set FEnableValue = *($(FEnableList), ~($(FEnableValues),$(FEnableIndex)))
		ifstr(i) $(FEnableValue) == ""
		set FEnableValue = *($(FEnableValues), 0)
		endif
    endif

    set InitDelayValue = *($(InitDelayList), ~($(InitDelayValues),$(InitDelayIndex)))
    ifstr(i) $(InitDelayValue) == ""
	set InitDelayValue = *($(InitDelayValues), 1)
    endif

    ifstr(i) $(EarlyTransmitValue) == ""
	set EarlyTransmitValue = 1
    endif

    ifstr(i) $(LinkIntegrityValue) == ""
	set LinkIntegrityValue = 1
    endif

    ifstr(i) $(DynamicLinkDetectValue) == ""
	set DynamicLinkDetectValue = 1
    endif

    ifint $(EarlyTransmitValue) == 1
	set EarlyTransmitValue = "ON"
    else
	set EarlyTransmitValue = "OFF"
    endif

    ifint $(LinkIntegrityValue) == 1
	set LinkIntegrityValue = "ON"
    else
	set LinkIntegrityValue = "OFF"
    endif

    ifint $(DynamicLinkDetectValue) == 1
	set DynamicLinkDetectValue = "ON"
    else
	set DynamicLinkDetectValue = "OFF"
    endif


    set CheckItemsIn = {$(EarlyTransmitValue),$(LinkIntegrityValue),$(DynamicLinkDetectValue)}
    ;set CheckItemsIn = {"ON", "ON", "OFF", "ON"}



    ;  Save the settings as they were read from the Registry.

;    Shell $(ParamInf) Param_SaveValues
;    Set CurrParamSettings = $($R0)
;
;   Put up the adapter configuration dialog if necessary.
;
;   Note that $(CurrParamSettings) has the old known parameter values.
;
adaptersetup = +


    ;Shell "" DebugConfiguration "before displaying dialog"

    Set from = adapteroptions

;   Verify that correct version of NT is present.
;   If not, display message and exit.
;
    LoadLibrary "disk 1" $(DialogDllName) hLib
    LibraryProcedure NTVersionShare, $(hLib), QueryNTVersion
    FreeLibrary $(hLib)
    ifint $(NTVersionShare) == 1
        read-syms NTVersionErrorDlg
        ui start "CustomMessageBox"
        goto end
    endif


adapteroptions = +

    set CheckItemsIn = {$(EarlyTransmitValue),$(LinkIntegrityValue),$(DynamicLinkDetectValue)}

    

	ifstr(i) $(CSInstalled) == "STANDARD NT4"
	
		set ENABLER = 0

		ifint $(RUNDLLCODE) == 1
				LibraryProcedure ENABLER, $(hLib), EnablerRunning 		; check for enabler type
				ifint $(ENABLER) == 1
					set Static1Label = "Configuring driver for Microsoft Enabler"
				else-ifint $(ENABLER) == 2
					set Static1Label = "Configuring driver for third party Card & Socket Services"
				 else
					set Static1Label = "Configuring driver for Xircom Enabler"
				 endif
		endif


		;------------------------------------------------------

		; Call out to the PCMCIA driver only if we're loading a PCMCIA device
		ifint $(RUNDLLCODE) == 1
				; DLLCODE
				; Locate the slot with the c56 card in it
				;------------------------------------------------------
				LibraryProcedure CONFIG, $(hLib), GetPCMCIAConfig
				set SLOTCOUNT = 8	; was 	*($(CONFIG),1), but returned 0
				set CONTROLLERTYPE = *($(CONFIG),3)
				;Debug-Output "slot count="$(SLOTCOUNT)" controller type="$(CONTROLLERTYPE)
				set SLOT = 0
			  slotloop = +
				LibraryProcedure INFO, $(hLib), GetVERS_1Tuple $(SLOT)      ;VERS_1
				ifstr(i) *($(INFO),3) == $(VERS1Manufacturer)
					ifstr(i) *($(INFO),4) == $(VERS1Product)
						goto slotfound
					endif
				endif

				set-add SLOT = $(SLOT), 1
				ifint $(SLOT) == $(SLOTCOUNT)
					goto slotnotfound
				else
					goto slotloop
				endif
			  slotfound = +
				;Debug-Output "c56 card found in slot "$(SLOT)
				;set Static2Label = "c56 in slot "$(SLOT)
				LibraryProcedure INFO, $(hLib), GetFUNCETuple $(SLOT)      ;VERS_1
				set	Static2Label = "Physical Address:"
				set	Static3Label = $(INFO)
				ifstr(i) $(NetworkAddressValue) != ""
				  set Static4Label = "Network Address:"
				  set Static5Label = $(NetworkAddressValue)
				endif
				set SLOTFOUND = 1
				goto slotcontinue
			  slotnotfound = +
				set SLOTFOUND = ""
				;set Static2Label = "c56 was not found"
				;Debug-Output "c56 card not found"
			  slotcontinue = +
		endif

	endif ;;;"STANDARD NT4"

	;------------------------------------------------------


	;
	; If this is an unattend installation we need to skip the DLL UI stuff.
	;
    ifstr(i) $(!STF_GUI_UNATTENDED) == "YES"
	goto skipoptions
    endif

	;;;===============================
	;;;-------start--Resource--Detect-----------------------------------------
	; display scanning message on initial install only, not in configure mode
	ifstr(i) $(CSInstalled) == "STANDARD NT4"
		Ifstr(i) $(!NTN_InstallMode) == install

			set DlgType			=	"MessageBox"
			set STF_MB_TITLE	=	"Xircom NT Resource Detect"
			set STF_MB_TEXT		=	"Resource Detect Completed successfully.  The hardware resources on the next screen are recommended to install the "$(GenericAdapterName)"."
			set STF_MB_TYPE		=	1
			set STF_MB_ICON		=	2
			set STF_MB_DEF		=	1

			ui start "Scanning Message"

		Endif
	endif

	;-----------------------------------------------
	; before dialog display
	; $(CurrParamSettings) values in Registry will be the default if currently installed

	set Curr_Memory			=	$(MemoryAddrValue)
	set Curr_MemValue			=	$(MemoryAddrIndex)
	set Curr_Io				=	$(IOBaseAddrValue)
	set Curr_IoValue				=	$(IOBaseAddrIndex)
	set Curr_Irq			=	$(IRQValue)
	set Curr_IrqValue			=	$(IRQValueIndex)
	set Curr_ComIo			=	$(ComIOBaseAddressValue)
	set Curr_ComIoValue			=	$(ComIOBaseAddressIndex)

	Ifstr(i) $(CSInstalled) == "Softex"
		set Curr_COMString		=	$(COMStringValue)
	Endif
	
		
	ifint $(RUNDLLCODE) == 1

		Set UsedIoList		= {}
		Set AvailIoList		= {}
		Set AvailIoValues	= {}

		Set UsedIrqList		= {}
		Set AvailIrqList	= {}
		Set AvailIrqValues	= {}

		Set UsedMemList		= {}
		Set AvailMemList	= {}
		Set AvailMemValues	= {}
		
		;========	start IO's	=================================
		
		;Scan for used Io port resources
		
		LibraryProcedure UsedIoList, $(hLib), GetResources "GetIoList"
		Debug-Output "UsedIoList: "$(UsedIoList)
		
		;all registered io resources found in Registry now reside in UsedIoList
		;--------------------------------------------------------
		;build the AvailIoList/Values based on results from Registry scan
		; then process UsedIoList against IOBaseAddrList/Values and ComIOBaseAddressList/Values

		Set AvailIoList			=	{}
		Set AvailIoValues		=	{}

		Set AvailComIoList		=	{}
		Set AvailComIoValues	=	{}
					
		Set Index = 0
		ForListDo $(IOBaseAddrList)						;;;Io ports that don't match the Used ones
			Set-add Index = $(Index), 1					;;;will become the new Available list

			Ifcontains(i) $($) not-in $(UsedIoList)
				Set AvailIoList = >($(AvailIoList), $($))
				Set AvailIoValues = >( $(AvailIoValues),  *($(IOBaseAddrValues), $(Index)) )
			Endif
		EndForListDo
		;;;Debug-Output "zz-AvailIoList: "$(AvailIoList)
		;;;Debug-Output "zz-AvailIoValues: "$(AvailIoValues)

		Set Index = 0
		ForListDo $(ComIOBaseAddressList)
			Set-add Index = $(Index), 1
			
			Ifcontains(i) $($) not-in $(UsedIoList)
				Set AvailComIoList = >($(AvailComIoList), $($))
				Set AvailComIoValues = >( $(AvailComIoValues),  *($(ComIOBaseAddressValues), $(Index)) )
			Endif
		EndForListDo

		;========================================================
		;now reassign AvailIoList/Values -> IOBaseAddrList/Values
		;also AvailComIoList/Values -> ComIOBaseAddressList/Values
		;

			Set IOBaseAddrList		=	{}
			Set IOBaseAddrValues	=	{}

			Set ComIOBaseAddressList		=	{}
			Set ComIOBaseAddressValues		=	{}

			ForListDo $(AvailIoList)
				Set IOBaseAddrList = >($(IOBaseAddrList), $($))
			EndForListDo
			
			ForListDo $(AvailIoValues)
				Set IOBaseAddrValues = >($(IOBaseAddrValues), $($))
			EndForListDo

			ForListDo $(AvailComIoList)
				Set ComIOBaseAddressList = >($(ComIOBaseAddressList), $($))
			EndForListDo

			ForListDo $(AvailComIoValues)
				Set ComIOBaseAddressValues = >($(ComIOBaseAddressValues), $($))
			EndForListDo
		
		;;;Debug-Output "now-AvailComIoList: "$(AvailComIoList)
		;;;Debug-Output "now-AvailComIoValues: "$(AvailComIoValues)
		;========	finished with IO's	=================================


		;========	start IRQs	=================================

		;scan for used Irq resources
		
		LibraryProcedure UsedIrqList, $(hLib), GetResources "GetIrqList"
		Debug-Output "UsedIrqList: "$(UsedIrqList)
		;--------------------------------------------------------
		;build the AvailIrqList/AvailIrqValues based on results from Registry scan
		
		Set Index = 0
		Set AvailIrqList = {}
		Set AvailIrqValues = {}

		ForListDo $(IRQList)								;;;Irqs that don't match the Used ones
			Set-add Index = $(Index), 1						;;;will become the new Available list
		
			Ifcontains(i) $($) not-in $(UsedIrqList)
				Set AvailIrqList = >($(AvailIrqList), $($))
				Set AvailIrqValues = >( $(AvailIrqValues),  *($(IRQValues), $(Index)) )
			Endif
		EndForListDo
		;--------------------------------------------------------
		;now reassign AvailIrqList -> IRQList and AvailIrqValues -> IRQValues
		
			Set IRQList = {}
			Set IRQValues = {}

			ForListDo $(AvailIrqList)
				Set IRQList = >($(IRQList), $($))
			EndForListDo

			ForListDo $(AvailIrqValues)
				Set IRQValues = >($(IRQValues), $($))
			EndForListDo
		;Debug-Output "IRQList: "$(IRQList)
		;Debug-Output "IRQValues: "$(IRQValues)
		;========	finished with IRQs	=================================


		;========	start MEM's	=================================
		;scan Registry for used Memory resources
		
		LibraryProcedure UsedMemList, $(hLib), GetResources "GetMemList"
		Debug-Output "UsedMemList: "$(UsedMemList)
		
		;--------------------------------------------------------
		;build the AvailMemList/Values based on results from Registry scan
		Set Index = 0
		Set AvailMemList = {}
		Set AvailMemValues = {}
		
		
		ForListDo $(MemoryAddrList)								;;;Mem ports that don't match the Used ones
			Set-add Index = $(Index), 1							;;;will become the new Available list
		
			Ifcontains(i) $($) not-in $(UsedMemList)
				Set AvailMemList = >($(AvailMemList), $($))
				Set AvailMemValues = >( $(AvailMemValues),  *($(MemoryAddrValues), $(Index)) )
			Endif
					
		EndForListDo
		
		;;;Debug-Output "now-AvailMemList: "$(AvailMemList)
		;;;Debug-Output "now-AvailMemValues: "$(AvailMemValues)
		
		;--------------------------------------------------------
		;now reassign AvailMemList/Values -> MemoryAddrList/Values
		
		;Debug-Output "MemListFlag: "$(MemListFlag)
				
			Set MemoryAddrList = {}
			Set MemoryAddrValues = {}
				
			ForListDo $(AvailMemList)
				Set MemoryAddrList = >($(MemoryAddrList), $($))
			EndForListDo

			ForListDo $(AvailMemValues)
				Set MemoryAddrValues = >($(MemoryAddrValues), $($))
			EndForListDo
		
		;;;Debug-Output "now-MemoryAddrList: "$(MemoryAddrList)
		;;;Debug-Output "now-MemoryAddrValues: "$(MemoryAddrValues)
		;========	finished with MEM's	=================================

	endif		;;;(RUNDLLCODE)


	
	;======================================================
	;;;in configure mode, currently installed CEM56 params from Registry is appended to Avail List/Values
	;;;since resource scan will exclude these as they are considered Used Resources

	Ifstr(i) $(!NTN_InstallMode) == "configure"
				
				Debug-Output "NTN_InstallMode == configure."
				Debug-Output "Curr_Io: "$(Curr_Io)
				Debug-Output "Curr_ComIo: "$(Curr_ComIo)
				Debug-Output "Curr_ComIoValue: "$(Curr_ComIoValue)
				Debug-Output "Curr_Irq: "$(Curr_Irq)
				Debug-Output "Curr_Memory: "$(Curr_Memory)

				Ifstr(i) $(CSInstalled) == "Softex"
					Debug-Output "Curr_COMString: "$(Curr_COMString)
				Endif

				ForListDo $(IOBaseAddrList)
					Ifcontains(i) $(Curr_Io) not-in $(IOBaseAddrList)
						Set IOBaseAddrList = >($(IOBaseAddrList),$(Curr_Io))
					Endif
					
					Ifcontains(i) $(Curr_IoValue) not-in $(IOBaseAddrValues)
						Set IOBaseAddrValues = >($(IOBaseAddrValues),$(Curr_IoValue))
					Endif
				EndForListDo
					;;;Debug-Output "YYY IOBaseAddrList: "$(IOBaseAddrList)
					;;;Debug-Output "YYY IOBaseAddrValues: "$(IOBaseAddrValues)

				ForListDo $(IRQList)
					Ifcontains(i) $(Curr_Irq) not-in $(IRQList)
						Set IRQList	= >($(IRQList),$(Curr_Irq))
					Endif
					Ifcontains(i) $(Curr_IrqValue) not-in $(IRQValues)
						Set IRQValues = >($(IRQValues), $(Curr_IrqValue))
					Endif
				EndForListDo
					;;;Debug-Output "YYY IRQList: "$(IRQList)
					;;;Debug-Output "YYY IRQValues: "$(IRQValues)
				
				ForListDo $(MemoryAddrList)
					Ifcontains(i) $(Curr_Memory) not-in $(MemoryAddrList)
						Set MemoryAddrList = >($(MemoryAddrList),$(Curr_Memory))
					Endif

					Ifcontains(i) $(Curr_MemValue) not-in $(MemoryAddrValues)
						Set MemoryAddrValues = >($(MemoryAddrValues),$(Curr_MemValue))
					Endif
				EndForListDo
					;;;Debug-Output "YYY MemoryAddrList: "$(MemoryAddrList)
					;;;Debug-Output "YYY MemoryAddrValues: "$(MemoryAddrValues)
				

				ForListDo $(ComIOBaseAddressList)
					Ifcontains(i) $(Curr_ComIo) not-in $(ComIOBaseAddressList)
						Set ComIOBaseAddressList = >($(ComIOBaseAddressList), $(Curr_ComIo))
						Debug-Output "added Curr_ComIo: "$(Curr_ComIo)
					Endif

					Ifcontains(i) $(Curr_ComIoValue) not-in $(ComIOBaseAddressValues)
						Set ComIOBaseAddressValues = >($(ComIOBaseAddressValues), $(Curr_ComIoValue))
						Debug-Output "added Curr_ComIoValue: "$(Curr_ComIoValue)
					Endif
				EndForListDo

				;;;Debug-Output "YYY ComIOBaseAddressList: "$(ComIOBaseAddressList)
				;;;Debug-Output "YYY ComIOBaseAddressValues: "$(ComIOBaseAddressValues)

	Endif
	;-----------------------------------------------
		;;;end Resource Detect
	;-----------------------------------------------


	ifstr(i) $(CSInstalled) == "Softex"
		read-syms FileDependentDlgSoftex$(!STF_LANGUAGE)"-"$(Option)
	else-ifstr(i) $(CSInstalled) == "STANDARD NT4"
		read-syms FileDependentDlg$(!STF_LANGUAGE)"-"$(Option)    
		;;;Debug-Output "read-syms FileDependentDlg$(!STF_LANGUAGE)-$(Option)"
	endif
	
	ui start "InputDlg"  $(hLib)

    set ExitButton      = $(ButtonPressed)

    FreeLibrary $(hLib)

    ifstr(i) $(DLGEVENT) == "CONTINUE"

	set IOBaseAddrIndex        = $(Combo1Out)
	set MemoryAddrIndex        = $(Combo2Out)
	set IRQValueIndex          = $(Combo3Out)
	set ModeIndex              = $(Combo4Out)
	set LineSpeedIndex         = $(Combo5Out)
	set LineModeIndex          = $(Combo6Out)
	set ComIOBaseAddressIndex  = $(Combo7Out)

	ifstr(i) $(CSInstalled) == "Softex"
		
		set COMStringIndex	   = $(Combo8Out)

	else-ifstr(i) $(CSInstalled) == "STANDARD NT4"

		set FEnableIndex	   = $(Combo8Out)
		set NdisVersionIndex		= $(Combo10Out)
		
	endif

	set InitDelayIndex	   = $(Combo9Out)
	set EarlyTransmitValue     = *($(CheckItemsOut), 1)
	set LinkIntegrityValue     = *($(CheckItemsOut), 2)
	set DynamicLinkDetectValue = *($(CheckItemsOut), 3)
	set ExitButton             = $(ButtonPressed)

	ui pop 1

    else-ifstr(i) $(DLGEVENT) == "EXIT"
	set CommonStatus = STATUS_USERCANCEL
	ui pop 1
	goto end
    else
	set CommonStatus = STATUS_USERCANCEL
	ui pop 1
	Debug-Output "Action: unknown. Bye."
	goto end
    endif


;
;   If installing, go create the necessary keys;
;   if configuring, they're already open.
;
skipoptions =+

	 ifint $(OldVersionExisted) == $(TRUE)
        ifstr(i) $(!NTN_InstallMode) == configure
            goto writeparameters
        endif
    endif
    StartWait
    ;
    ; Add Software Component
    ;
    ifint $(OldVersionExisted) == $(FALSE)

        ifstr(i) $(!NTN_InstallMode) == "install"
           Ifstr(i) $(DoCopy) == "YES"

				  Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) YES

              Ifint $($ShellCode) != $(!SHELL_CODE_OK)
                  Goto ShellCodeError
              Else-Ifstr(i) $($R0) == STATUS_FAILED
                  Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
                  ifint $($ShellCode) != $(!SHELL_CODE_OK)
							 goto ShellCodeError
                  endif
                  set Error = $($R0)
                  Goto fatal
              Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
                  Goto successful
              Endif

              Set SrcDir = $($R1)

           Endif

           install "Install-Option"

			  ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
              Shell $(UtilityInf) RegistryErrorString "UNABLE_COPY_FILE"
              ifint $($ShellCode) != $(!SHELL_CODE_OK)
                  goto ShellCodeError
              endif
              set Error = $($R0)
              goto fatal
			  endif
        endif



        Shell $(UtilityInf), AddSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), +
				$(ProductSoftwareName), +
            $(ProductSoftwareTitle), $(STF_CONTEXTINFNAME), +
            $(ProductSoftwareImagePath), "kernel", "NDIS", {}, "",+
            $(NetEventDLL)

        Set OEM_ABANDON_SOFTWARE = TRUE

		  ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif
        ;
        ;   At this point:
        ;     $R1 contains the product version key handle;
	;     $R2 contains the NetRules subkey handle;
        ;     $R3 contains the new Services key handle; and
        ;     $R4 contains the Parameters key
        ;     $R5 contains the Linkage Key
        ;
        set RegistryErrorIndex = $($R0)
        set KeyProduct      = $($R1)
		  Set SoftNetRulesKey = $($R2)
        CloseRegKey $($R3)
        CloseRegKey $($R4)
        CloseRegKey $($R5)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            EndWait
				Debug-Output "Registry error: add software components"
            CloseRegKey $(KeyProduct)
            CloseRegKey $(SoftNetRulesKey)
            goto fatalregistry
        endif

        set NewValueList = {{SoftwareType,$(NoTitle),$(!REG_VT_SZ),$(SoftwareType)},+
                           {MajorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMajorVersion)},+
                           {MinorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMinorVersion)},+
                           {Title,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareTitle)},+
                           {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareDescription)},+
                           {ServiceName,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareName)},+
                           {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

		  Shell  $(UtilityInf), AddValueList, $(KeyProduct), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error."
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            EndWait
            Debug-Output "Registry error: add value list."
            CloseRegKey $(KeyProduct)
            CloseRegKey $(SoftNetRulesKey)
            goto fatalregistry
		  endif

        set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareType)},+
                            {use,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareUse)}, +
                            {bindform,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareBindForm)}, +
                            {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareClass)}, +
                            {bindable,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareBindable)}, +
									 {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

        Shell  $(UtilityInf), AddValueList, $(SoftNetRulesKey), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error."
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        CloseRegKey $(KeyProduct)
        CloseRegKey $(SoftNetRulesKey)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
				EndWait
            Debug-Output "Resgitry error: add value list."
            goto fatalregistry
        endif
    endif
;
;   Create the HARDWARE\Netcard region and its corresponding service
;
    Shell $(UtilityInf), AddHardwareComponent, $(ProductHardwareName),$(STF_CONTEXTINFNAME),$(ProductKeyName)

    ifint $($R4) != -1
        Set OEM_ABANDON_OPTIONS = >($(OEM_ABANDON_OPTIONS), $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards\"$($R4))
    endif

	 ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "Cannot add hardware component"
        goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

	 Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
        EndWait
        Debug-Output "Registry error: add hardware component"
        CloseRegKey $($R1)
        CloseRegKey $($R2)
        CloseRegKey $($R3)
        goto fatalregistry
	 endif

;
;   At this point:
;     $R1  Registry key variable for HARDWARE\Netcard\(n)
;     $R2  Registry key variable for HARDWARE\Netcard\(n)\\NetRules
;     $R3  Registry key handle for <service>\Parameters key
;     $R4  Adapter number assigned to adapter
;     $R5  Service name generated by combining svc name with adapter number
;
    set KeyParameters = $($R3)
    set KeyAdapterRules = $($R2)
    set AdapterNumber = $($R4)

	 set NewValueList = {{Manufacturer,$(NoTitle),$(!REG_VT_SZ),$(Manufacturer)},+
                       {Title,$(NoTitle),$(!REG_VT_SZ),"["$($R4)"] "$(ProductHardwareTitle)},+
                       {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareDescription)},+
                       {ProductName,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
                       {ServiceName,$(NoTitle),$(!REG_VT_SZ),$($R5)},+
                       {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

	 Shell  $(UtilityInf), AddValueList, $($R1), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error"
        goto ShellCodeError
    endif

    CloseRegKey $($R1)

    set TempProdName = """"$(ProductHardwareName)$(AdapterNumber)""""
    set TempBindForm = $(TempProdName)$(NetRuleHardwareBindForm)

    set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleHardwareType)},+
                        {bindform,$(NoTitle),$(!REG_VT_SZ),$(TempBindForm)}, +
                        {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleHardwareClass)}, +
								{InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

    Shell  $(UtilityInf), AddValueList, $(KeyAdapterRules), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error."
        goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
        EndWait
        Debug-Output "Resgitry error: add value list."
        CloseRegKey $(KeyParameters)
		  CloseRegKey $(KeyAdapterRules)
        goto fatalregistry
    endif

    CloseRegKey $(KeyAdapterRules)

    goto writeparameters
;
;   REQUIRED:   $(KeyParameters) contains service Parameters key handle
;
writeparameters = +
;    Shell $(UtilityInf), GetBusTypeNum
;    set BusTypeNum = $($R1)

; Following line is set to 1 (for ISA) to accomodate PCI machines which
; are sometimes reported to be BusType 5 (PCI).
    set BusTypeNum = 1
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error."
        goto ShellCodeError
    endif

;
;   Add the rest of the parameters to the Services area
;
    ifstr(i) $(EarlyTransmitValue) == "ON"
	set EarlyTransmitValue =  "1"
    else
	set EarlyTransmitValue =  "0"
    endif

    ifstr(i) $(LinkIntegrityValue) == "ON"
	set LinkIntegrityValue =  "1"
    else
	set LinkIntegrityValue =  "0"
    endif

    ifstr(i) $(DynamicLinkDetectValue) == "ON"
	set DynamicLinkDetectValue =  "1"
    else
	set DynamicLinkDetectValue =  "0"
    endif

    ifstr(i) $(!STF_GUI_UNATTENDED) == "YES"
		ifstr(i) $(CSInstalled) == "Softex"
			set ModeValue                  = *($(ModeValues), 1)
			set MemoryAddrValue            = *($(MemoryAddrValues), $(DEFAULT_LANMEM))
			set-add CommonMemoryAddrValue  = $(MemoryAddrValue),   8192
			set IRQValue                   = *($(IRQValues), $(DEFAULT_IRQ))
			set IOBaseAddrValue            = *($(IOBaseAddrValues), $(DEFAULT_LANIO))
			set ComIOBaseAddressValue      = *($(ComIOBaseAddressValues), $(DEFAULT_MDMIO))
			set COMStringValue              = *($(COMStringValues), $(DEFAULT_COM)) ;
			set LineSpeedValue             = *($(LineSpeedValues), 1)
			set LineModeValue              = *($(LineModeValues), 1)
			set InitDelayValue	       = *($(InitDelayValues), 1)
			set IOLengthValue              = 15

		else-ifstr(i) $(CSInstalled) == "STANDARD NT4"
			set ModeValue                  = *($(ModeValues), 1)
			set MemoryAddrValue            = *($(MemoryAddrValues), 53)
			set-add CommonMemoryAddrValue  = $(MemoryAddrValue),   8192
			set IRQValue                   = *($(IRQValues), 8)
			set IOBaseAddrValue            = *($(IOBaseAddrValues), 18)
			set ComIOBaseAddressValue      = *($(ComIOBaseAddressValues), 4)
			set LineSpeedValue             = *($(LineSpeedValues), 1)
			set LineModeValue              = *($(LineModeValues), 1)
			set FEnableValue               = *($(FEnableValues), 1)
			set InitDelayValue	       = *($(InitDelayValues), 1)
			set NdisVersionValue	       = *($(NdisVersionValues), 1)
			set IOLengthValue              = 15
		endif
    else
		ifstr(i) $(CSInstalled) == "Softex"
			set ModeValue                  = *($(ModeValues),      ~($(ModeList),       $(ModeIndex)))
			set MemoryAddrValue            = *($(MemoryAddrValues),~($(MemoryAddrList), $(MemoryAddrIndex)))
			set-add CommonMemoryAddrValue  = $(MemoryAddrValue),   8192
			set IRQValue                   = *($(IRQValues),       ~($(IRQList),        $(IRQValueIndex)))
			set IOBaseAddrValue            = *($(IOBaseAddrValues),~($(IOBaseAddrList), $(IOBaseAddrIndex)))
			set ComIOBaseAddressValue      = *($(ComIOBaseAddressValues),~($(ComIOBaseAddressList), $(ComIOBaseAddressIndex)))
			set COMStringValue              = *($(COMStringValues), ~($(COMStringList), $(COMStringIndex))) ;
			set LineSpeedValue             = *($(LineSpeedValues), ~($(LineSpeedList),  $(LineSpeedIndex)))
			set LineModeValue              = *($(LineModeValues),  ~($(LineModeList),   $(LineModeIndex)))
			set InitDelayValue		= *($(InitDelayValues),    ~($(InitDelayList),     $(InitDelayIndex)))
			set IOLengthValue              = 15
		else-ifstr(i) $(CSInstalled) == "STANDARD NT4"
			set ModeValue                  = *($(ModeValues),      ~($(ModeList),       $(ModeIndex)))
			set MemoryAddrValue            = *($(MemoryAddrValues),~($(MemoryAddrList), $(MemoryAddrIndex)))
			set-add CommonMemoryAddrValue  = $(MemoryAddrValue),   8192
			set IRQValue                   = *($(IRQValues),       ~($(IRQList),        $(IRQValueIndex)))
			set IOBaseAddrValue            = *($(IOBaseAddrValues),~($(IOBaseAddrList), $(IOBaseAddrIndex)))
			set ComIOBaseAddressValue      = *($(ComIOBaseAddressValues),~($(ComIOBaseAddressList), $(ComIOBaseAddressIndex)))
			set LineSpeedValue             = *($(LineSpeedValues), ~($(LineSpeedList),  $(LineSpeedIndex)))
			set LineModeValue              = *($(LineModeValues),  ~($(LineModeList),   $(LineModeIndex)))
			set FEnableValue               = *($(FEnableValues),   ~($(FEnableList),    $(FEnableIndex)))
			set InitDelayValue	       = *($(InitDelayValues),    ~($(InitDelayList),     $(InitDelayIndex)))
			set NdisVersionValue	       = *($(NdisVersionValues),    ~($(NdisVersionList),     $(NdisVersionIndex)))
			set IOLengthValue              = 15
		endif
	endif

	ifstr(i) $(CSInstalled) == "Softex"

		set NewValueList = {{BusNumber,               $(NoTitle),$(!REG_VT_DWORD),0},+
								{BusType,                 $(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
								{ComNumber,               $(NoTitle), $(!REG_VT_SZ), $(COMStringValue)},+  
								;{DirectEnable,            $(NoTitle),$(!REG_VT_DWORD),$(DirectEnableValue)},+
								{DynamicLinkDetect,       $(NoTitle),$(!REG_VT_DWORD),$(DynamicLinkDetectValue)},+
								{EarlyTransmit,           $(NoTitle),$(!REG_VT_DWORD),$(EarlyTransmitValue)},+
								{InitDelay,		      $(NoTitle),$(!REG_VT_DWORD),$(InitDelayValue)},+
								{InterruptNumber,         $(NoTitle),$(!REG_VT_DWORD),$(IRQValue)},+
								{IoBaseAddress,           $(NoTitle),$(!REG_VT_DWORD),$(ComIOBaseAddressValue)},+
								{IoLength,                $(NoTitle),$(!REG_VT_DWORD), 7},+
								{IoBaseAddress_1,         $(NoTitle),$(!REG_VT_DWORD),$(IOBaseAddrValue)},+
								{IoLength_1,              $(NoTitle),$(!REG_VT_DWORD), 15},+
								{LineSpeed,               $(NoTitle),$(!REG_VT_DWORD),$(LineSpeedValue)},+
								{LineMode,                $(NoTitle),$(!REG_VT_DWORD),$(LineModeValue)},+
								{LinkIntegrity,           $(NoTitle),$(!REG_VT_DWORD),$(LinkIntegrityValue)},+
								{MemoryMappedBaseAddress, $(NoTitle),$(!REG_VT_DWORD),$(CommonMemoryAddrValue)},+
								{MemoryMappedSize,        $(NoTitle),$(!REG_VT_DWORD),4096},+
								{MediaType,               $(NoTitle),$(!REG_VT_DWORD),1},+
								{Mode,                    $(NoTitle),$(!REG_VT_DWORD),$(ModeValue)},+
								{ModemFunction,                $(NoTitle),$(!REG_VT_DWORD), 1},+
								{PCCARDAttributeMemoryAddress, $(NoTitle),$(!REG_VT_DWORD),$(MemoryAddrValue)},+
								{PCCARDAttributeMemoryOffset,  $(NoTitle),$(!REG_VT_DWORD),61440},+
								{PCCARDAttributeMemorySize,    $(NoTitle),$(!REG_VT_DWORD),8192},+
								{PCCARDMemoryWindowOffset,     $(NoTitle),$(!REG_VT_DWORD),0},+
								;{PCMCIA,                  $(NoTitle),$(!REG_VT_DWORD),$(PcmciaValue)},+
								{PlatformType,            $(NoTitle),$(!REG_VT_DWORD), 0},+
								{ProductName,             $(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
								{SoftexPcmcia,            $(NoTitle),$(!REG_VT_DWORD), 1},+
								{TransmitBufferSize,      $(NoTitle),$(!REG_VT_DWORD),7168}}

	else-ifstr(i) $(CSInstalled) == "STANDARD NT4"

		set NewValueList = {{BusNumber,               $(NoTitle),$(!REG_VT_DWORD),0},+
								{BusType,                 $(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
								{DynamicLinkDetect,       $(NoTitle),$(!REG_VT_DWORD),$(DynamicLinkDetectValue)},+
								{EarlyTransmit,           $(NoTitle),$(!REG_VT_DWORD),$(EarlyTransmitValue)},+
								{FunctionEnable,          $(NoTitle),$(!REG_VT_DWORD),$(FEnableValue)},+
					{InitDelay,		      $(NoTitle),$(!REG_VT_DWORD),$(InitDelayValue)},+
					{NdisVersion,		      $(NoTitle),$(!REG_VT_DWORD),$(NdisVersionValue)},+
								{InterruptNumber,         $(NoTitle),$(!REG_VT_DWORD),$(IRQValue)},+
								{IoBaseAddress,           $(NoTitle),$(!REG_VT_DWORD),$(ComIOBaseAddressValue)},+
								{IoLength,                $(NoTitle),$(!REG_VT_DWORD), 7},+
								{IoBaseAddress_1,         $(NoTitle),$(!REG_VT_DWORD),$(IOBaseAddrValue)},+
								{IoLength_1,              $(NoTitle),$(!REG_VT_DWORD), 15},+
								{LineSpeed,               $(NoTitle),$(!REG_VT_DWORD),$(LineSpeedValue)},+
								{LineMode,                $(NoTitle),$(!REG_VT_DWORD),$(LineModeValue)},+
								{LinkIntegrity,           $(NoTitle),$(!REG_VT_DWORD),$(LinkIntegrityValue)},+
								{MemoryMappedBaseAddress, $(NoTitle),$(!REG_VT_DWORD),$(CommonMemoryAddrValue)},+
								{MemoryMappedSize,        $(NoTitle),$(!REG_VT_DWORD),4096},+
								{MediaType,               $(NoTitle),$(!REG_VT_DWORD),1},+
								{Mode,                    $(NoTitle),$(!REG_VT_DWORD),$(ModeValue)},+
								{ModemFunction,                $(NoTitle),$(!REG_VT_DWORD), 1},+
								{PCCARDAttributeMemoryAddress, $(NoTitle),$(!REG_VT_DWORD),$(MemoryAddrValue)},+
								{PCCARDAttributeMemoryOffset,  $(NoTitle),$(!REG_VT_DWORD),61440},+
								{PCCARDAttributeMemorySize,    $(NoTitle),$(!REG_VT_DWORD),8192},+
								{PCCARDMemoryWindowOffset,     $(NoTitle),$(!REG_VT_DWORD),0},+
								{PCMCIA,                  $(NoTitle),$(!REG_VT_DWORD),1},+
								{PlatformType,            $(NoTitle),$(!REG_VT_DWORD), 0},+
								{TransmitBufferSize,      $(NoTitle),$(!REG_VT_DWORD),7168}}
	endif	;;;"STANDARD NT4"



    Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)

    ;
    ; If unattended install, update the registry with the values from the unattend.txt file.
    ;
    ifstr(i) $(!STF_GUI_UNATTENDED) == "YES"
	Shell $(UtilityInf), AddDefaultNetCardParameters, $(KeyParameters)

	;
	; Now read back the values just written to the registry so we can configure the slot
	; later (if necessary).
	;
	set ValueList = {}
	EnumRegValue $(KeyParameters) ValueList
	ForListDo $(ValueList)
	    set ValueItem = $($)
	    set ValueName = *($(ValueItem),1)
	    set ValueData = *($(ValueItem),4)
	    ifstr(i) $(ValueName) == "InterruptNumber"
	        set IRQValue = $(ValueData)
	
	    else-ifstr(i) $(ValueName) == "IoBaseAddress_1"
	        set IOBaseAddrValue = $(ValueData)
	
	    else-ifstr(i) $(ValueName) == "PCCARDAttributeMemoryAddress"
	        set MemoryAddrValue = $(ValueData)
	
	    endif
	EndForListDo
    endif

    CloseRegKey $(KeyParameters)

    ifstr(i) $(CSInstalled) == "STANDARD NT4"
	
			;;;----START---Ndis Switch---------------------

			ifint $(NdisVersionValue) == "1"		;;;Ndis 3
				
				OpenRegKey $(!REG_H_LOCAL) "" "SYSTEM\CurrentControlSet\Services\"$(ProductSoftwareName) $(MAXIMUM_ALLOWED) ImagePathHandle
		
				Ifstr $(ImagePathHandle) != $(KeyNull)
					SetRegValue $(ImagePathHandle) {ImagePath, 0, $(!REG_VT_SZ), "\SystemRoot\System32\drivers\CEM56.sys"}
				Endif
				CloseRegKey $(ImagePathHandle)

			else-ifint $(NdisVersionValue) == "0"		;;;Ndis 4
		
				OpenRegKey $(!REG_H_LOCAL) "" "SYSTEM\CurrentControlSet\Services\"$(ProductSoftwareName) $(MAXIMUM_ALLOWED) ImagePathHandle
		
				Ifstr $(ImagePathHandle) != $(KeyNull)
					SetRegValue $(ImagePathHandle) {ImagePath, 0, $(!REG_VT_SZ), "\SystemRoot\System32\drivers\CEM56N4.sys"}
				Endif
				CloseRegKey $(ImagePathHandle)
			endif
			;;;----END---Ndis Switch----------------------

		; --------------------------------------------------------------------------------
		; Reprogram the PCMCIA slot with the new parameters.  This should only be done
		; during first time installation of NT and/or networking, and if our adapter 
		; has been found.  This should not occur if the user is simply reconfiguring a
		; previously installed adapter that is up and running.
		; --------------------------------------------------------------------------------

		ifstr(i) $(!NTN_InstallMode) != configure
		ifint $(RUNDLLCODE) == 1
			ifint $(ENABLER) == 1
				ifint $(HOTPROGRAMPCMCIA) == 1
					ifint $(SLOTFOUND) == 1
						
						; Add our adapter to the hardware description section of the
						; registry.  This will allow the driver to start running
						; during NT or network installation.
		
						set PCMCIASYSTEMKeyName = "HARDWARE\DESCRIPTION\System"
						set PCMCIAPCCARDSKeyName = $(PCMCIASYSTEMKeyName)"\PCMCIA PCCARDs"
		
						OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIASYSTEMKeyName) $(!REG_KEY_CREATE_SUB_KEY) SYSTEMKeyHandle
						ifstr $(SYSTEMKeyHandle) != $(NULL)
							CreateRegKey $(SYSTEMKeyHandle) {"PCMCIA PCCARDs", 0, 0} "" $(!REG_KEY_SET_VALUE) 0 PCCARDsKeyHandle
							ifstr $(PCCARDsKeyHandle) != $(NULL)
								SetRegValue $(PCCARDsKeyHandle) {$(ProductSoftwareName), 0, $(!REG_VT_DWORD), 0}
								CloseRegKey $(PCCARDsKeyHandle)
								Debug-Output "CEM56 INF - PCMCIA PCCARDs key created, name/value pair set"
							else
								Debug-Output "CEM56 INF - PCMCIA PCCARDs key already exists"
							endif
							CloseRegKey $(SYSTEMKeyHandle)
						endif
						
						LoadLibrary "disk 1" $(DialogDllName) hLib
						Debug-Output "Enabling network resources"
						LibraryProcedure STATUS, $(hLib), SetupSlot $(SLOT) $(IRQValue) 0 $(IOBaseAddrValue) $(IOLengthValue) $(MemoryAddrValue) 4096 61440
						Debug-Output "SetupSlot: "$(STATUS)
						FreeLibrary $(hLib)
					endif
				endif
			endif
		endif
		endif
    
		; --------------------------------------------------------------------------------
		; Write the parameters to the PCMCIA database section, iff running MS Enabler
		; Add/replace only the parts for the c56
		; --------------------------------------------------------------------------------
		set PCMCIADatabaseKeyName = $(!NTN_ServiceBase)"\Pcmcia\DataBase"
	;   set PCMCIADatabaseMfgKeyName = $(PCMCIADatabaseKeyName)"\"$(VERS1Manufacturer)
		set PCMCIADatabaseMfgKeyName = $(PCMCIADatabaseKeyName)"\Xircom"
		OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseKeyName) $(MAXIMUM_ALLOWED) PCMCIADatabaseKey

		ifstr $(PCMCIADatabaseKey) == $(NULL)
		;Debug-Output "Pcmcia\DataBase not present"
		else ; PCMCIA.sys is installed and registry has database section in it.
		; Try to open Manufacturer section.  Delete it if found
	;	OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseKeyName)"\"$(VERS1Manufacturer) $(MAXIMUM_ALLOWED) PCMCIADatabaseMfgKey
		OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseKeyName)"\Xircom" $(MAXIMUM_ALLOWED) PCMCIADatabaseMfgKey
		ifstr $(PCMCIADatabaseMfgKey) == $(NULL) ; open failed, so create Manufacturer subkey
	;		CreateRegKey $(PCMCIADatabaseKey) {$(VERS1Manufacturer), 0, 0} "" $(MAXIMUM_ALLOWED) "" PCMCIADatabaseMfgKey
			CreateRegKey $(PCMCIADatabaseKey) {"Xircom", 0, 0} "" $(MAXIMUM_ALLOWED) "" PCMCIADatabaseMfgKey
		endif

		; Open "Ethernet 10/100"  aka $(VERS1Product) ----------------------------------------------------------------------
    		OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseMfgKeyName)"\"$(VERS1Product) $(MAXIMUM_ALLOWED) PCMCIADatabaseMfgC56Key
		ifstr $(PCMCIADatabaseMfgC56Key) == $(NULL)
			CreateRegKey $(PCMCIADatabaseMfgKey) {$(VERS1Product), 0, 0} "" $(MAXIMUM_ALLOWED) 0 PCMCIADatabaseMfgC56Key
		endif

		; Set the values --------------------------------------------------------------------------------------
		SetRegValue $(PCMCIADatabaseMfgC56Key) {Driver, 0, $(!REG_VT_SZ),"CEM56"}
		SetRegValue $(PCMCIADatabaseMfgC56Key) {AttributeMemorySize, 0, $(!REG_VT_DWORD),8192}
		SetRegValue $(PCMCIADatabaseMfgC56Key) {DeviceType, 0, $(!REG_VT_SZ),"NET"}
		CloseRegKey $(PCMCIADatabaseMfgC56Key)
		CloseRegKey $(PCMCIADatabaseMfgKey)
		CloseRegKey $(PCMCIADatabaseKey)
		endif

		
		; --------------------------------------------------------------------------------
		; --------------------------------------------------------------------------------
	endif	;;;"STANDARD NT4"

    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error."
        goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
        Debug-Output "Registry error: Add value list"
        goto fatalregistry
    endif

    EndWait

    goto successful

;-----------------------------------------------
; Binding section
;-----------------------------------------------
bindingadapter =+
    set Error = "Binding: Sorry, not yet implemented."
    goto fatal

;-----------------------------------------------
; Removeadapter section
;-----------------------------------------------

removeadapter = +
    Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
        ; Remove Software Component
        Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    else
        Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), $(!NTN_RegBase)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif


    endif

    goto end

;-----------------------------------------------
; Upgrade Software section
;-----------------------------------------------

UpgradeSoftware = +
    ;
    ; First determine whether we want to do upgrade or update for software
    ; or hardware component. Then we will determine whether the Mode is
    ; update or upgrade.
    ;
    ; If the same version of the product existed in the registry, we do
    ; update. Otherwise, we will do a upgrade
    ;
    ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
        ; Upgrade software component
        ;
        ; see whether the same version exist or not
        ;
        OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

        Ifstr $(KeyProduct) != $(KeyNull)
            GetRegValue $(KeyProduct),"MajorVersion", VersionInfo
            set Version = *($(VersionInfo), 4)

            ;
            ; Update the binaries
            ;
            Shell $(UtilityInf), GetInfFileNameFromRegistry, $(KeyProduct)

            ifint $($ShellCode) != $(!SHELL_CODE_OK)
                Debug-Output "ShellCode error"
                goto ShellCodeError
            endif

            set !UG_Filename = $($R0)

            ifstr(i) $(!UG_Filename) != ""
                install "Install-Update"
                ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
                    goto fatal
                endif
            endif

            ; Upgrade the version number
            ;
            SetRegValue $(KeyProduct) {MajorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMajorVersion)}
            SetRegValue $(KeyProduct) {MinorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMinorVersion)}

            ;
            ; do nothing for update
            ;
            ifint $(Version) != $(ProductVersion)
               ;
               ; If the major version number is not the same,
               ; it is major upgrade. So let Upgrade the product
               ;
               ;
               ; make other upgrade change if necessary
               ;
            endif
            CloseRegKey $(KeyProduct)
        else
            ;
            ; Cannot Open software key, goto ERROR
            ;
            goto fatalregistry
        endif
    else
        ;
        ; upgrade/update hardware component
        ; There is no different between upgrade and update for hardware
        ; component
        ;
        ; 1. Get the Service Name
        ; 2. Change the NetRule section if necessary
        ;
        OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) +
              $(MAXIMUM_ALLOWED) NetworkCardKey
        Ifstr(i) $(NetworkCardKey) != $(KeyNull)
            ;
            ; Get Service name
            ;
            GetRegValue $(NetworkCardKey),"ServiceName", ServiceNameInfo
            set ServiceName = *($(ServiceNameInfo), 4)

            ;
            ; Change the NetRule if necessary
            ;
            OpenRegKey $(NetworkCardKey) "" "NetRules" +
                $(MAXIMUM_ALLOWED) NetRuleKey
            Ifstr(i) $(NetRuleKey) != $(KeyNull)
                ;
                ; Make the change....
                ;
            else
                ;
                ; Error, cannot open net rules key
                ;
                goto fatalregistry
            endif

            CloseRegKey $(NetRules)
            CloseRegKey $(NetworkCardKey)
        else
            ;
            ; Error, cannot open network card key
            ;
            goto fatalregistry
        endif
        ;
        ; 3. Change the service section of the hardware. i.e.,
        ;    ParameterName change, value change, etc.
        ;
        OpenRegKey $(!REG_H_LOCAL) "" +
              $(!NTN_ServiceBase)"\"$(ServiceName) +
              $(MAXIMUM_ALLOWED) ServiceKey

        Ifstr(i) $(ServiceKey) != $(KeyNull)
            ;
            ; Get the ServiceKey to change the Start value
            ; or Type value. Or open Parameters key to
            ; change the hardware parameters if necessary.
            ;
            CloseRegKey $(ServiceKey)
        else
            ;
            ; Error, cannot open network card key
            ;
            goto fatalregistry
        endif
    endif

    goto end
    ;
    ; End of Upgrade Software
    ;

;
;  Escape hatches
;
successful = +
    goto end

abandon = +
    ForListDo $(OEM_ABANDON_OPTIONS)
        Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), $($)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    EndForListDo

    Ifstr(i) $(OEM_ABANDON_SOFTWARE) == TRUE
        ; Remove Software Component
        Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), FALSE
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    endif

    goto end

;
; warning display
;
warning = +
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "WARNING", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
        goto $(to)
    else-ifstr(i) $($R1) == "CANCEL"
        goto $(from)
    else
        goto "end"
    endif
;
; non fatal error display
;
nonfatalinfo = +
    Set Severity = STATUS
    Set CommonStatus = STATUS_USERCANCEL
    goto nonfatalmsg
nonfatal = +
    Set Severity = NONFATAL
    goto nonfatalmsg
nonfatalmsg = +
    ifstr(i) $(Error) == ""
        Set Severity = NONFATAL
        Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), $(Severity), $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
        goto $(from)
    else
        goto "end"
    endif

;
;  Registry is broken
;
fatalregistry = +
    Shell $(UtilityInf) RegistryErrorString $(RegistryErrorIndex)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    set Error = $($R0)
    goto fatal
;
;  Netcard detection failure
;
fataldetect = +
    Shell $(UtilityInf),RegistryErrorString,CANNOT_DETECT
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error: cannot get an error string."
        goto ShellCodeError
    endif
    set Error = $($R0)
    Goto fatal
;
; fatal error display
;
fatal = +
    ifstr(i) $(Error) == ""
        Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "FATAL", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif

    goto setfailed

;
;  Shelling error
;
ShellCodeError = +
    set DlgType      = "MessageBox"
    set STF_MB_TITLE = $(ShellCodeErrorTitle)
    set STF_MB_TEXT  = $(ShellCodeErrorText)
    set STF_MB_TYPE  = 1
    set STF_MB_ICON  = 3
    set STF_MB_DEF   = 1
    ui start "Error Message"
    goto setfailed

setfailed = +
    set CommonStatus = STATUS_FAILED
    ;
    ; if OEM_ABANDON_ON == TRUE, then remove the registry entries
    ;
    ifstr(i) $(OEM_ABANDON_ON) == TRUE
        set OEM_ABANDON_ON = FALSE
        goto abandon
    endif
    goto end

end = +
    goto term

term = +

    Return $(CommonStatus)

[DebugConfiguration]

    Set InfName = "OEMSETNT.INF"
    ;Debug-Output $(InfName)" **CONFIGURATION STATE: "$($0)
    ;Debug-Output $(InfName)" IRQ_Level is "$(!p:IRQ_Level)
    ;Debug-Output $(InfName)" IOBaseAddrValue is "$(!p:IOBaseAddrValue)
    ;Debug-Output $(InfName)" TransceiverValue is "$(!p:TransceiverValue)
    ;Debug-Output $(InfName)" MemoryAddr is "$(!p:MemoryAddr)
    ;Debug-Output $(InfName)" MappedValue is "$(!p:MappedValue)

    return


;***************************************************************
;  INSTALL SECTIONS
;***************************************************************
[Install-Option]
    set STF_VITAL = ""

	ifstr(i) $(AddCopy) == "YES"

		ifstr(i) $(CSInstalled) == "Softex"

		  AddSectionFilesToCopyList FilesSoftex-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers

		else-ifstr(i) $(CSInstalled) == "STANDARD NT4"

		  AddSectionFilesToCopyList FilesN4-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
		  AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers

		endif

		AddSectionFilesToCopyList Files-MdmRASInf $(SrcDir) $(!STF_WINDOWSPATH)\drivers
		AddSectionFilesToCopyList Files-MdmInf $(SrcDir) $(!STF_WINDOWSPATH)\inf

	endif

	;BCM

	 ifstr(i) $(DoCopy) == "YES"

       ;
       ; Copy files in the copy list
		 ;
       set !STF_NCPA_FLUSH_COPYLIST = TRUE
       CopyFilesInCopyList

    endif

    Exit

[Install-Update]
	set STF_VITAL        = ""
	set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
	;set STF_VERSION     = "YES"

	ifstr(i) $(CSInstalled) == "Softex"

		AddSectionFilesToCopyList FilesSoftex-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers

	else-ifstr(i) $(CSInstalled) == "STANDARD NT4"

		AddSectionFilesToCopyList FilesN4-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
		AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers

	endif

	AddSectionFilesToCopyList Files-Inf $(SrcDir) $(!STF_WINDOWSSYSPATH)
	AddSectionFilesToCopyList Files-MdmInf $(SrcDir) $(!STF_WINDOWSPATH)\inf
	AddSectionFilesToCopyList Files-MdmRASInf $(SrcDir) $(!STF_WINDOWSPATH)\drivers

	set !STF_NCPA_FLUSH_COPYLIST = TRUE
	CopyFilesInCopyList

	exit


[Install-Dll]
	set STF_VITAL 	= ""
	AddSectionFilesToCopyList Files-Dll $(SrcDir) $(!STF_WINDOWSSYSPATH)
	set !STF_NCPA_FLUSH_COPYLIST = TRUE
	CopyFilesInCopyList
	exit





[Source Media Descriptions]
    1  = "Windows 95, 98, NT Installation Disk for Xircom Ethernet 10/100+Modem 56"


[ProductType]
STF_PRODUCT  = Winnt
STF_PLATFORM = I386


[Files-Inf]
1, OEMSETNT.INF, SIZE=58000,	RENAME=$(!UG_Filename)

[Files-MdmInf]
1, MDMCEM56.INF, SIZE=15000

[Files-MdmRASInf]
1, MODEM.IN_, SIZE=255000, BACKUP=MODEM.BAK, DESTINATION=$(!STF_WINDOWSSYSPATH)\RAS DECOMPRESS RENAME=MODEM.INF

[Files-Dll]
1, CEM56.DLL,  SIZE=21000

[FilesN4-CEM56]
1, CEM56N4.SYS, SIZE=33000

[FilesSoftex-CEM56]
1, CEM56NT.SYS, SIZE=33000

[Files-CEM56]
1, CEM56.SYS, SIZE=33000

[LanguagesSupported]
	 ENG

[AllFileConstantsENG]
ProCaption   = "Windows NT Setup"
ProCancel    = "Cancel"
ProCancelMsg = "Windows NT Networking is not correctly installed.  "+
               "Are you sure you want to cancel copying files?"
ProCancelCap = "Network Setup Message"
ProText1     = "Copying:"
ProText2     = "To:"
DialogDllName     = "CEM56.DLL"



; START c56 -------------------------------------------------------------------------------------------

;;;----------START---FileConstantsSoftexENG-CEM56----------;;;
[FileConstantsSoftexENG-CEM56]
FunctionTitle		= $(GenericAdapterName)" Setup"$(GenericInfVersion)
ProductSoftwareTitle	= $(GenericDriverName)
ProductHardwareTitle	= $(GenericAdapterName)
IRQList			= ^(IRQChoicesSoftex, 1)
IRQValues		= ^(IRQChoicesSoftex, 2)
IOBaseAddrList		= ^(IOBaseAddrChoicesSoftex, 1)
IOBaseAddrValues	= ^(IOBaseAddrChoicesSoftex, 2)
MemoryAddrList		= ^(MemoryAddrChoicesSoftex,1)
MemoryAddrValues	= ^(MemoryAddrChoicesSoftex,2)
ModeList		= ^(ModeChoices, 1)
ModeValues		= ^(ModeChoices, 2)
LineSpeedList		= ^(LineSpeedChoices, 1)
LineSpeedValues		= ^(LineSpeedChoices, 2)
LineModeList		= ^(LineModeChoices, 1)
LineModeValues		= ^(LineModeChoices, 2)
ComIOBaseAddressList	= ^(ComIOBaseAddressChoicesSoftex,1)
ComIOBaseAddressValues	= ^(ComIOBaseAddressChoicesSoftex,2)
InitDelayList           = ^(InitDelayChoices, 1)
InitDelayValues         = ^(InitDelayChoices, 2)
COMStringList		= ^(COMStringChoices,1)		
COMStringValues		= ^(COMStringChoices,2)		
;;;---------END---FileConstantsSoftexENG-CEM56----------;;;


;;;----------START---FileConstantsENG-CEM56----------;;;
[FileConstantsENG-CEM56]
FunctionTitle		= $(GenericAdapterName)" Setup"$(GenericInfVersion)
ProductSoftwareTitle	= $(GenericDriverName)
ProductHardwareTitle	= $(GenericAdapterName)
IRQList			= ^(IRQChoices, 1)
IRQValues		= ^(IRQChoices, 2)
IOBaseAddrList		= ^(IOBaseAddrChoices, 1)
IOBaseAddrValues	= ^(IOBaseAddrChoices, 2)
MemoryAddrList		= ^(MemoryAddrChoices,1)
MemoryAddrValues	= ^(MemoryAddrChoices,2)
ModeList		= ^(ModeChoices, 1)
ModeValues		= ^(ModeChoices, 2)
LineSpeedList		= ^(LineSpeedChoices, 1)
LineSpeedValues		= ^(LineSpeedChoices, 2)
LineModeList		= ^(LineModeChoices, 1)
LineModeValues		= ^(LineModeChoices, 2)
ComIOBaseAddressList	= ^(ComIOBaseAddressChoices,1)
ComIOBaseAddressValues	= ^(ComIOBaseAddressChoices,2)
FEnableList		= ^(FEnableChoices, 1)
FEnableValues		= ^(FEnableChoices, 2)
InitDelayList           = ^(InitDelayChoices, 1)
InitDelayValues         = ^(InitDelayChoices, 2)
NdisVersionList           = ^(NdisVersionChoices, 1)
NdisVersionValues         = ^(NdisVersionChoices, 2)
;;;--------END---FileConstantsENG-CEM56----------;;;

[DialogConstantsENG-CEM56]
Help        = "&Help"
Exit        = "Cancel"
OK          = "OK"
HelpContext = ""
Continue    = "Continue"
Cancel      = "Cancel"

;;;-----------START---FileDependentDlgSoftexENG-CEM56-----;;;
[FileDependentDlgSoftexENG-CEM56]
DlgType = "RadioCombination"
DlgTemplate = "CEM56_3"
Caption = $(FunctionTitle)
HelpContext = $(!IDH_DB_OEMNADE2_INS)
CBOptionsGreyed = {}
NotifyFields = {NO, NO, NO, NO, NO, NO, NO, NO}
Combo1Label = "I/O Port:"
Combo2Label = "Memory Address:"
Combo3Label = "Interrupt:"
Combo4Label = "Mode:"
Combo5Label = "Line Speed:"
Combo6Label = "Line Mode:"
Combo7Label = "I/O Port:"
Combo8Label = "COM Number:"
Combo9Label = "Initialization Delay:"
Check1 = "&Early Transmit"
Check2 = "Link &Integrity"
;Check3 = "&Direct Enable"
Check3 = "Dynamic &Link Detect"
Combo1List = $(IOBaseAddrList)
Combo1Out  = $(IOBaseAddrValue)
Combo2List = $(MemoryAddrList)
Combo2Out  = $(MemoryAddrValue)
Combo3List = $(IRQList)
Combo3Out  = $(IRQValue)
Combo4List = $(ModeList)
Combo4Out  = $(ModeValue)
Combo5List = $(LineSpeedList)
Combo5Out  = $(LineSpeedValue)
Combo6List = $(LineModeList)
Combo6Out  = $(LineModeValue)
Combo7List = $(ComIOBaseAddressList)
Combo7Out  = $(ComIOBaseAddressValue)
Combo8List = $(COMStringList)
Combo8Out = $(COMStringValue)
Combo9List = $(InitDelayList)
Combo9Out  = $(InitDelayValue)

ComboListItemsIn  = {Combo1List,Combo2List,Combo3List, Combo4List, Combo5List, Combo6List, Combo7List, Combo8List, Combo9List}
ComboListItemsOut = {Combo1Out, Combo2Out, Combo3Out, Combo4Out, Combo5Out, Combo6Out, Combo7Out, Combo8Out, Combo9Out}
CheckItemsIn = {$(EarlyTransmitValue),$(LinkIntegrityValue),$(DynamicLinkDetectValue)}
; Does the next line do anything?
CheckItemsOut = {Check1Out, Check2Out, Check3Out}
EditTextIn  = {"",""}
EditTextLim = {"",""}
;;;--------END---FileDependentDlgSoftexENG-CEM56-----;;;


;;;-----------START---FileDependentDlgENG-CEM56-----;;;
[FileDependentDlgENG-CEM56]
DlgType = "RadioCombination"
DlgTemplate = "CEM56_1"
Caption = $(FunctionTitle)
HelpContext = $(!IDH_DB_OEMNADE2_INS)
CBOptionsGreyed = {}
NotifyFields = {NO, NO, NO, NO, NO, NO, NO, NO, NO}
Combo1Label = "I/O Port:"
Combo2Label = "Memory Address:"
Combo3Label = "Interrupt:"
Combo4Label = "Mode:"
Combo5Label = "Line Speed:"
Combo6Label = "Line Mode:"
Combo7Label = "I/O Port:"
Combo8Label = "Function(s):"
Combo9Label = "Initialization Delay:"
Combo10Label = "Ndis Version:"
Check1 = "&Early Transmit"
Check2 = "Link &Integrity"
Check3 = "Dynamic &Link Detect"
Combo1List = $(IOBaseAddrList)
Combo1Out  = $(IOBaseAddrValue)
Combo2List = $(MemoryAddrList)
Combo2Out  = $(MemoryAddrValue)
Combo3List = $(IRQList)
Combo3Out  = $(IRQValue)
Combo4List = $(ModeList)
Combo4Out  = $(ModeValue)
Combo5List = $(LineSpeedList)
Combo5Out  = $(LineSpeedValue)
Combo6List = $(LineModeList)
Combo6Out  = $(LineModeValue)
Combo7List = $(ComIOBaseAddressList)
Combo7Out  = $(ComIOBaseAddressValue)
Combo8List = $(FEnableList)
Combo8Out  = $(FEnableValue)
Combo9List = $(InitDelayList)
Combo9Out  = $(InitDelayValue)
Combo10List = $(NdisVersionList)
Combo10Out  = $(NdisVersionValue)
ComboListItemsIn  = {Combo1List,Combo2List,Combo3List, Combo4List, Combo5List, Combo6List, Combo7List, Combo8List, Combo9List, Combo10List}
ComboListItemsOut = {Combo1Out, Combo2Out, Combo3Out, Combo4Out, Combo5Out, Combo6Out, Combo7Out, Combo8Out, Combo9Out, Combo10Out}
CheckItemsIn = {$(EarlyTransmitValue),$(LinkIntegrityValue),$(DynamicLinkDetectValue)}
CheckItemsOut = {Check1Out, Check2Out, Check3Out}
EditTextIn  = {"",""}
EditTextLim = {"",""}
;;;-------END---FileDependentDlgENG-CEM56-----;;;

[NTVersionErrorDlg]
DlgType      = "MessageBox"
STF_MB_TITLE = "Xircom Ethernet 10/100+Modem 56 Setup Message"
STF_MB_TEXT  = "Please see the readme.txt for instructions on NT3.51 Installation."
STF_MB_TYPE  = 1
STF_MB_ICON  = 3
STF_MB_DEF   = 1

; END c56 -------------------------------------------------------------------------------------------

;;;----------START---MemoryAddrChoicesSoftex-----;;;
[MemoryAddrChoicesSoftex]
MA_0  = "Auto Detect", 4294967295
MA_1  = "0xA0000", 655360
MA_2  = "0xA1000", 659456
MA_3  = "0xA2000", 663552
MA_4  = "0xA3000", 667648
MA_5  = "0xA4000", 671744
MA_6  = "0xA5000", 675840
MA_7  = "0xA6000", 679936
MA_8  = "0xA7000", 684032
MA_9  = "0xA8000", 688128
MA_10 = "0xA9000", 692224
MA_11 = "0xAA000", 696320
MA_12 = "0xAB000", 700416
MA_13 = "0xAC000", 704512
MA_14 = "0xAD000", 708608
MA_15 = "0xAE000", 712704
MA_16 = "0xAF000", 716800
MA_17 = "0xB0000", 720896
MA_18 = "0xB1000", 724992
MA_19 = "0xB2000", 729088
MA_20 = "0xB3000", 733184
MA_21 = "0xB4000", 737280
MA_22 = "0xB5000", 741376
MA_23 = "0xB6000", 745472
MA_24 = "0xB7000", 749568
MA_25 = "0xB8000", 753664
MA_26 = "0xB9000", 757760
MA_27 = "0xBA000", 761856
MA_28 = "0xBB000", 765952
MA_29 = "0xBC000", 770048
MA_30 = "0xBD000", 774144
MA_31 = "0xBE000", 778240
MA_32 = "0xBF000", 782336
MA_33 = "0xC0000", 786432
MA_34 = "0xC1000", 790528
MA_35 = "0xC2000", 794624
MA_36 = "0xC3000", 798720
MA_37 = "0xC4000", 802816
MA_38 = "0xC5000", 806912
MA_39 = "0xC6000", 811008
MA_40 = "0xC7000", 815104
MA_41 = "0xC8000", 819200
MA_42 = "0xC9000", 823296
MA_43 = "0xCA000", 827392
MA_44 = "0xCB000", 831488
MA_45 = "0xCC000", 835584
MA_46 = "0xCD000", 839680
MA_47 = "0xCE000", 843776
MA_48 = "0xCF000", 847872
MA_49 = "0xD0000", 851968
MA_50 = "0xD1000", 856064
MA_51 = "0xD2000", 860160
MA_52 = "0xD3000", 864256
MA_53 = "0xD4000", 868352
MA_54 = "0xD5000", 872448
MA_55 = "0xD6000", 876544
MA_56 = "0xD7000", 880640
MA_57 = "0xD8000", 884736
MA_58 = "0xD9000", 888832
MA_59 = "0xDA000", 892928
MA_60 = "0xDB000", 897024
MA_61 = "0xDC000", 901120
MA_62 = "0xDD000", 905216
MA_63 = "0xDE000", 909312
MA_64 = "0xDF000", 913408
MA_65 = "0xE0000", 917504
MA_66 = "0xE1000", 921600
MA_67 = "0xE2000", 925696
MA_68 = "0xE3000", 929792
MA_69 = "0xE4000", 933888
MA_70 = "0xE5000", 937984
MA_71 = "0xE6000", 942080
MA_72 = "0xE7000", 946176
MA_73 = "0xE8000", 950272
MA_74 = "0xE9000", 954368
MA_75 = "0xEA000", 958464
MA_76 = "0xEB000", 962560
MA_77 = "0xEC000", 966656
MA_78 = "0xED000", 970752
MA_79 = "0xEE000", 974848
MA_80 = "0xEF000", 978944
MA_81 = "0xF0000", 983040
MA_82 = "0xF1000", 987136
MA_83 = "0xF2000", 991232
MA_84 = "0xF3000", 995328
MA_85 = "0xF4000", 999424
MA_86 = "0xF5000", 1003520
MA_87 = "0xF6000", 1007616
MA_88 = "0xF7000", 1011712
MA_89 = "0xF8000", 1015808
MA_90 = "0xF9000", 1019904
MA_91 = "0xFA000", 1024000
MA_92 = "0xFB000", 1028096
MA_93 = "0xFC000", 1032192
;MA_94 = "0xFD000", 1036288
;MA_95 = "0xFE000", 1040384
;;;-------END---MemoryAddrChoicesSoftex-----;;;


;;;----------START---MemoryAddrChoices-----;;;
[MemoryAddrChoices]
MA_1  = "0xA0000", 655360
MA_2  = "0xA1000", 659456
MA_3  = "0xA2000", 663552
MA_4  = "0xA3000", 667648
MA_5  = "0xA4000", 671744
MA_6  = "0xA5000", 675840
MA_7  = "0xA6000", 679936
MA_8  = "0xA7000", 684032
MA_9  = "0xA8000", 688128
MA_10 = "0xA9000", 692224
MA_11 = "0xAA000", 696320
MA_12 = "0xAB000", 700416
MA_13 = "0xAC000", 704512
MA_14 = "0xAD000", 708608
MA_15 = "0xAE000", 712704
MA_16 = "0xAF000", 716800
MA_17 = "0xB0000", 720896
MA_18 = "0xB1000", 724992
MA_19 = "0xB2000", 729088
MA_20 = "0xB3000", 733184
MA_21 = "0xB4000", 737280
MA_22 = "0xB5000", 741376
MA_23 = "0xB6000", 745472
MA_24 = "0xB7000", 749568
MA_25 = "0xB8000", 753664
MA_26 = "0xB9000", 757760
MA_27 = "0xBA000", 761856
MA_28 = "0xBB000", 765952
MA_29 = "0xBC000", 770048
MA_30 = "0xBD000", 774144
MA_31 = "0xBE000", 778240
MA_32 = "0xBF000", 782336
MA_33 = "0xC0000", 786432
MA_34 = "0xC1000", 790528
MA_35 = "0xC2000", 794624
MA_36 = "0xC3000", 798720
MA_37 = "0xC4000", 802816
MA_38 = "0xC5000", 806912
MA_39 = "0xC6000", 811008
MA_40 = "0xC7000", 815104
MA_41 = "0xC8000", 819200
MA_42 = "0xC9000", 823296
MA_43 = "0xCA000", 827392
MA_44 = "0xCB000", 831488
MA_45 = "0xCC000", 835584
MA_46 = "0xCD000", 839680
MA_47 = "0xCE000", 843776
MA_48 = "0xCF000", 847872
MA_49 = "0xD0000", 851968
MA_50 = "0xD1000", 856064
MA_51 = "0xD2000", 860160
MA_52 = "0xD3000", 864256
MA_53 = "0xD4000", 868352
MA_54 = "0xD5000", 872448
MA_55 = "0xD6000", 876544
MA_56 = "0xD7000", 880640
MA_57 = "0xD8000", 884736
MA_58 = "0xD9000", 888832
MA_59 = "0xDA000", 892928
MA_60 = "0xDB000", 897024
MA_61 = "0xDC000", 901120
MA_62 = "0xDD000", 905216
MA_63 = "0xDE000", 909312
MA_64 = "0xDF000", 913408
MA_65 = "0xE0000", 917504
MA_66 = "0xE1000", 921600
MA_67 = "0xE2000", 925696
MA_68 = "0xE3000", 929792
MA_69 = "0xE4000", 933888
MA_70 = "0xE5000", 937984
MA_71 = "0xE6000", 942080
MA_72 = "0xE7000", 946176
MA_73 = "0xE8000", 950272
MA_74 = "0xE9000", 954368
MA_75 = "0xEA000", 958464
MA_76 = "0xEB000", 962560
MA_77 = "0xEC000", 966656
MA_78 = "0xED000", 970752
MA_79 = "0xEE000", 974848
MA_80 = "0xEF000", 978944
MA_81 = "0xF0000", 983040
MA_82 = "0xF1000", 987136
MA_83 = "0xF2000", 991232
MA_84 = "0xF3000", 995328
MA_85 = "0xF4000", 999424
MA_86 = "0xF5000", 1003520
MA_87 = "0xF6000", 1007616
MA_88 = "0xF7000", 1011712
MA_89 = "0xF8000", 1015808
MA_90 = "0xF9000", 1019904
MA_91 = "0xFA000", 1024000
MA_92 = "0xFB000", 1028096
MA_93 = "0xFC000", 1032192
MA_94 = "0xFD000", 1036288
MA_95 = "0xFE000", 1040384
;;;------END---MemoryAddrChoices-----;;;

;;;----------START---IRQChoicesSoftex-----;;;
[IRQChoicesSoftex]
;Interrupts available on the PCIC: { 3,4,5,7,8,10,11,12,14,15 }
;Interrupts available on the TCIC: { 3,4,5,6,7,10,14 }
;6  = floppy disk
;12 = keyboard
;14 = fixed disk
IRQ_0 = "Auto Detect", 0
IRQ_1 = "3",3
IRQ_2 = "4",4
IRQ_3 = "5",5
IRQ_4 = "7",7
IRQ_5 = "8",8
IRQ_6 = "9",9
IRQ_7 = "10",10
IRQ_8 = "11",11
IRQ_9 = "15",15
;;;------END---IRQChoicesSoftex-----;;;

;;;----------START---IRQChoices-----;;;
[IRQChoices]
;Interrupts available on the PCIC: { 3,4,5,7,8,10,11,12,14,15 }
;Interrupts available on the TCIC: { 3,4,5,6,7,10,14 }
;6  = floppy disk
;12 = keyboard
;14 = fixed disk
IRQ_1 = "3",3
IRQ_2 = "4",4
IRQ_3 = "5",5
IRQ_4 = "7",7
IRQ_5 = "8",8
IRQ_6 = "9",9
IRQ_7 = "10",10
IRQ_8 = "11",11
IRQ_9 = "15",15
;;;------END---IRQChoices-----;;;


[ModeChoices]
MO_1 = "I/O", 0
MO_2 = "Memory Mapped", 1

;;;----------START---ComIOBaseAddressChoicesSoftex-----;;;
[ComIOBaseAddressChoicesSoftex]
; Using list from Cardbus with range 100 to 200 added
; 0x3E0 is where PCIC is located
; 0x240 is where TCIC is located
MIOBase_0  = "Auto Detect", 65535	; DEFAULT_MDMIO choice
MIOBase_1  = "0x3F8",1016
MIOBase_2  = "0x2F8",760
MIOBase_3  = "0x3E8",1000
MIOBase_4  = "0x2E8",744   
MIOBase_40  = "0x100", 256
MIOBase_41  = "0x110",272
MIOBase_42  = "0x120",288
MIOBase_43  = "0x130",304
MIOBase_44 = "0x140",320
MIOBase_45  = "0x150",336
MIOBase_46  = "0x160",352
MIOBase_47  = "0x170",368
MIOBase_48  = "0x180",384
MIOBase_49  = "0x190",400
MIOBase_4A  = "0x1A0",416
MIOBase_4B  = "0x1B0",432
MIOBase_4C  = "0x1C0",448
MIOBase_4D  = "0x1D0",464
MIOBase_4E  = "0x1E0",480
MIOBase_4F  = "0x1F0",496
MIOBase_5  = "0x200",512
MIOBase_6  = "0x210",528
MIOBase_7  = "0x220",544
MIOBase_8  = "0x230",560
;MIOBase_9  = "0x240",576
MIOBase_10 = "0x250",592
MIOBase_11 = "0x260",608
MIOBase_12 = "0x270",624
MIOBase_13 = "0x280",640
MIOBase_14 = "0x290",656
MIOBase_15 = "0x2A0",672
MIOBase_16 = "0x2B0",698
MIOBase_17 = "0x2C0",714
MIOBase_18 = "0x2D0",730
MIOBase_19 = "0x2E0",746
MIOBase_20 = "0x2F0",752
MIOBase_21 = "0x300",768
MIOBase_22 = "0x310",784
MIOBase_23 = "0x320",800
MIOBase_24 = "0x330",816
MIOBase_25 = "0x340",832
MIOBase_26 = "0x350",848
MIOBase_27 = "0x360",864
MIOBase_28 = "0x370",880
MIOBase_29 = "0x380",896
MIOBase_30 = "0x390",912
MIOBase_31 = "0x3A0",928
MIOBase_32 = "0x3B0",944
MIOBase_33 = "0x3C0",960
MIOBase_34 = "0x3D0",976

;ComIOBase_0  = "Auto Detect", 65535
;ComIOBase_1  = "0x3F8",1016
;ComIOBase_2  = "0x2F8",760
;ComIOBase_3  = "0x3E8",1000
;ComIOBase_4  = "0x2E8",744
;;;-----END---ComIOBaseAddressChoicesSoftex-----;;;


;;;----------START---ComIOBaseAddressChoices-----;;;
[ComIOBaseAddressChoices]
ComIOBase_1  = "0x3F8",1016
ComIOBase_2  = "0x2F8",760
ComIOBase_3  = "0x3E8",1000
ComIOBase_4  = "0x2E8",744
;;;----END--ComIOBaseAddressChoices-----;;;

[LineSpeedChoices]
LS_1 = "Auto Detect", 0
LS_2 = "10 Mbps", 1
LS_3 = "100 Mbps", 2

[LineModeChoices]
LM_1 = "Auto Detect", 0
LM_2 = "Half Duplex", 1
LM_3 = "Full Duplex", 2

[FEnableChoices]
FEnable_1 = "Network & Modem", 0
FEnable_2 = "Network only", 1
FEnable_3 = "Modem only", 2

;;;---------START---IOBaseAddrChoicesSoftex-----;;;
[IOBaseAddrChoicesSoftex]
; 0x3E0 is where PCIC is located
; 0x240 is where TCIC is located
; therefore user cannot select these for locating the ethernet adapter
IOBase_0  = "Auto Detect", 65535
IOBase_1  = "0x200",512
IOBase_2  = "0x210",528
IOBase_3  = "0x220",544
IOBase_4  = "0x230",560
;IOBase_5  = "0x240",576
IOBase_6  = "0x250",592
IOBase_7  = "0x260",608
IOBase_8  = "0x270",624
IOBase_9  = "0x280",640
IOBase_10 = "0x290",656
IOBase_11 = "0x2A0",672
IOBase_12 = "0x2B0",698
IOBase_13 = "0x2C0",714
IOBase_14 = "0x2D0",730
IOBase_15 = "0x2E0",746
IOBase_16 = "0x2F0",752
IOBase_17 = "0x300",768
IOBase_18 = "0x310",784
IOBase_19 = "0x320",800
IOBase_20 = "0x330",816
IOBase_21 = "0x340",832
IOBase_22 = "0x350",848
IOBase_23 = "0x360",864
IOBase_24 = "0x370",880
IOBase_25 = "0x380",896
IOBase_26 = "0x390",912
IOBase_27 = "0x3A0",928
IOBase_28 = "0x3B0",944
IOBase_29 = "0x3C0",960
IOBase_30 = "0x3D0",976
;;;----END---IOBaseAddrChoicesSoftex-----;;;


;;;---------START---IOBaseAddrChoices-----;;;
[IOBaseAddrChoices]
; 0x3E0 is where PCIC is located
; 0x240 is where TCIC is located
; therefore user cannot select these for locating the ethernet adapter
IOBase_1  = "0x200",512
IOBase_2  = "0x210",528
IOBase_3  = "0x220",544
IOBase_4  = "0x230",560
;IOBase_5  = "0x240",576
IOBase_6  = "0x250",592
IOBase_7  = "0x260",608
IOBase_8  = "0x270",624
IOBase_9  = "0x280",640
IOBase_10 = "0x290",656
IOBase_11 = "0x2A0",672
IOBase_12 = "0x2B0",698
IOBase_13 = "0x2C0",714
IOBase_14 = "0x2D0",730
IOBase_15 = "0x2E0",746
IOBase_16 = "0x2F0",752
IOBase_17 = "0x300",768
IOBase_18 = "0x310",784
IOBase_19 = "0x320",800
IOBase_20 = "0x330",816
IOBase_21 = "0x340",832
IOBase_22 = "0x350",848
IOBase_23 = "0x360",864
IOBase_24 = "0x370",880
IOBase_25 = "0x380",896
IOBase_26 = "0x390",912
IOBase_27 = "0x3A0",928
IOBase_28 = "0x3B0",944
IOBase_29 = "0x3C0",960
IOBase_30 = "0x3D0",976
;;;----END---IOBaseAddrChoices-----;;;

[COMStringChoices]
;CS_0 = "AutoDetect", 0	  ; Later for Auto
CS_1 = "COM1", COM1
CS_2 = "COM2", COM2
CS_3 = "COM3", COM3
CS_4 = "COM4", COM4
CS_5 = "COM5", COM5
CS_6 = "COM6", COM6
CS_7 = "COM7", COM7
CS_8 = "COM8", COM8

[InitDelayChoices]
InitD_0 = "0",0
InitD_1 = "1",1
InitD_2 = "2",2
InitD_3 = "3",3
InitD_4 = "4",4
InitD_5 = "5",5
InitD_6 = "10",10
InitD_7 = "20",20
InitD_8 = "30",30
InitD_9 = "40",40
InitD_10 = "50",50
InitD_11 = "60",60

[NdisVersionChoices]
NV_1 = "NDIS 4", 0
NV_2 = "NDIS 3", 1
