; Copyright (c) 1993-1995 Microsoft Corporation

;*** IMPORTANT ***: If you modify the section related to real-mode driver removal, also update subase.inf accordingly.
; Section to look at (PCMCIA under BaseWinOptions)

[Version]
CatalogFile=pcmcia.cat
Signature="$CHICAGO$"
LayoutFile=Layout.inf, Layout1.inf, Layout2.inf
Class=PCMCIA
ClassGUID={4d36e977-e325-11ce-bfc1-08002be10318}
Provider=%MS%

;
;   Information for installing the PCMCIA class
;
[ClassInstall]
AddReg=ClassAddReg

[ClassAddReg]
HKR,,,,%ClassName%
HKR,,Installer,,MSPCIC.dll
HKR,,Icon,,0
HKR,,EnumPropPages,,"MSPCIC.dll, EnumClassPropPages"

;
;   List of manufacturers and devices
;
[Manufacturer]
%MS%=MS
%GenDrvs%=Generic
%IBMMfg%=IBM
%IntelMfg%=Intel
%DatabookMfg%=DATABOOK
%SMC%=SMC
%VLSIMfg%=VLSI
%CompaqMfg%=Compaq
%CirrusMfg%=Cirrus
%VademMfg%=Vadem
%MXTR%=Maxtor
%SCM%=SCM
%TI%=TI
%Toshiba%=Toshiba
%OPTi%=OPTi
%Ricoh%=Ricoh
%Trident%=Trident
%O2MicroMfg%=O2Micro

[MS]
%PCCard.DeviceDesc%=NODRV,PCCARD
%PCCard.DeviceDesc%=NODRV,PCMCIA\PCCARD
%PCI\CC_0607.DeviceDesc%=CARDBUS, PCI\CC_0607

[NODRV]

[ControlFlags]
ExcludeFromSelect=PCCARD
ExcludeFromSelect=PCMCIA\PCCARD
ExcludeFromSelect=PCI\CC_0607
ExcludeFromSelect=PCI\VEN_8086&DEV_1221
ExcludeFromSelect=PCI\VEN_10B3&DEV_3106
ExcludeFromSelect=PCI\VEN_10B8&DEV_B106
ExcludeFromSelect=PCI\VEN_1013&DEV_1100
ExcludeFromSelect=PCI\VEN_1013&DEV_1110
ExcludeFromSelect=PCI\VEN_1013&DEV_1112
ExcludeFromSelect=PCI\VEN_1013&DEV_1113
ExcludeFromSelect=PCI\VEN_1179&DEV_060A
ExcludeFromSelect=PCI\VEN_1179&DEV_060F
ExcludeFromSelect=PCI\VEN_104C&DEV_AC12
ExcludeFromSelect=PCI\VEN_104C&DEV_AC15
ExcludeFromSelect=PCI\VEN_104C&DEV_AC13
ExcludeFromSelect=PCI\VEN_104C&DEV_AC16
ExcludeFromSelect=PCI\VEN_104C&DEV_AC17
ExcludeFromSelect=PCI\VEN_104C&DEV_AC18
ExcludeFromSelect=PCI\VEN_104C&DEV_AC19
ExcludeFromSelect=PCI\VEN_104C&DEV_AC1A
ExcludeFromSelect=PCI\VEN_104C&DEV_AC1D
ExcludeFromSelect=PCI\VEN_1045&DEV_C824
ExcludeFromSelect=PCI\VEN_1045&DEV_C814
ExcludeFromSelect=PCI\VEN_1180&DEV_0466
ExcludeFromSelect=PCI\VEN_1180&DEV_0465
ExcludeFromSelect=PCI\VEN_1180&DEV_0476
ExcludeFromSelect=PCI\VEN_1180&DEV_0478
ExcludeFromSelect=PCI\VEN_1180&DEV_0475
ExcludeFromSelect=PCI\VEN_119B&DEV_1221
ExcludeFromSelect=PCI\VEN_119B&DEV_1221
ExcludeFromSelect=PCI\VEN_1023&DEV_0194
ExcludeFromSelect=PCI\VEN_1217&DEV_6729
ExcludeFromSelect=PCI\VEN_1217&DEV_673a
ExcludeFromSelect=PCI\VEN_1217&DEV_6832
ExcludeFromSelect=PCI\VEN_1217&DEV_6836
CopyFilesOnly=*DBK0402
CopyFilesOnly=*DBK1402
CopyFilesOnly=*DBK0214
CopyFilesOnly=*CPQA0DE
CopyFilesOnly=*VDM0469
CopyFilesOnly=*SCM0469
CopyFilesOnly=*IBM0030

[Generic]
%GenPCIC%=PCIC,*PNP0E00

[IBM]
%*IBM0030.DeviceDesc%=PCIC,*IBM0030

[Intel]
%IntelProto%=PCIC,,*PNP0E00
%IntelPCI%=PCIC,PCI\VEN_8086&DEV_1221

[Compaq]
%*CPQA0DE.DeviceDesc%=VLELC,*CPQA0DE,*PNP0E02

[DATABOOK]
%*DBK0000.DeviceDesc%=DBK0000,*DBK0000
%*DBK0402.DeviceDesc%=DBK0402,*DBK0402
%*DBK0204.DeviceDesc%=DBK0402,*DBK0204
%*DBK1402.DeviceDesc%=DBK1402,*DBK1402
%*DBK0214.DeviceDesc%=DBK1402,*DBK0214
%PCI\VEN_10B3&DEV_3106.DeviceDesc%=DBKCARDBUS, PCI\VEN_10B3&DEV_3106

[SMC]
%PCI\VEN_10B8&DEV_B106.DeviceDesc%=DBKCARDBUS, PCI\VEN_10B8&DEV_B106

[Maxtor]
%MXTR.Deskrunner%=DBK0000,*DBK0000

[VLSI]
%*PNP0E02.DeviceDesc%=VLELC,*PNP0E02

[Cirrus]
%Cirrus.DeviceDesc%=PCIC,*PNP0E01,*PNP0E00
%PCI\VEN_1013&DEV_1100.DeviceDesc%=PCIC, PCI\VEN_1013&DEV_1100
%PCI\VEN_1013&DEV_1110.DeviceDesc%=CLCARDBUS, PCI\VEN_1013&DEV_1110
%PCI\VEN_1013&DEV_1112.DeviceDesc%=CLCARDBUS, PCI\VEN_1013&DEV_1112
%PCI\VEN_1013&DEV_1113.DeviceDesc%=CLCARDBUS, PCI\VEN_1013&DEV_1113

[Vadem]
%Vadem.DeviceDesc%=PCIC,,*PNP0E00
%*VDM0469.DeviceDesc%=PCIC,*VDM0469

[SCM]
%SCM.DeviceDesc%=PCIC,,*PNP0E00
%*SCM0469.DeviceDesc%=PCIC,*SCM0469

[Toshiba]
%PCI\VEN_1179&DEV_060A.DeviceDesc%=TOPIC, PCI\VEN_1179&DEV_060A
%PCI\VEN_1179&DEV_060F.DeviceDesc%=TOPIC, PCI\VEN_1179&DEV_060F

[TI]
%PCI\VEN_104C&DEV_AC12.DeviceDesc%=TICARDBUS, PCI\VEN_104C&DEV_AC12
%PCI\VEN_104C&DEV_AC13.DeviceDesc%=TICARDBUS, PCI\VEN_104C&DEV_AC13
%PCI\VEN_104C&DEV_AC15.DeviceDesc%=TICARDBUS, PCI\VEN_104C&DEV_AC15
%PCI\VEN_104C&DEV_AC16.DeviceDesc%=TICARDBUS, PCI\VEN_104C&DEV_AC16
%PCI\VEN_104C&DEV_AC17.DeviceDesc%=TICARDBUS, PCI\VEN_104C&DEV_AC17
%PCI\VEN_104C&DEV_AC18.DeviceDesc%=TICARDBUS, PCI\VEN_104C&DEV_AC18
%PCI\VEN_104C&DEV_AC19.DeviceDesc%=TICARDBUS, PCI\VEN_104C&DEV_AC19
%PCI\VEN_104C&DEV_AC1A.DeviceDesc%=TICARDBUS, PCI\VEN_104C&DEV_AC1A
%PCI\VEN_104C&DEV_AC1B.DeviceDesc%=NTICARDBUS, PCI\VEN_104C&DEV_AC1B
%PCI\VEN_104C&DEV_AC1D.DeviceDesc%=TICARDBUS, PCI\VEN_104C&DEV_AC1D
%PCI\VEN_104C&DEV_AC1C.DeviceDesc%=NTICARDBUS, PCI\VEN_104C&DEV_AC1C

[OPTi]
%PCI\VEN_1045&DEV_C824.DeviceDesc%=OPTICARDBUS, PCI\VEN_1045&DEV_C824
%PCI\VEN_1045&DEV_C814.DeviceDesc%=OPTICARDBUS, PCI\VEN_1045&DEV_C814

[Ricoh]
%PCI\VEN_1180&DEV_0466.DeviceDesc%=RICOHCARDBUS, PCI\VEN_1180&DEV_0466
%PCI\VEN_1180&DEV_0465.DeviceDesc%=RICOHCARDBUS, PCI\VEN_1180&DEV_0465
%PCI\VEN_1180&DEV_0476.DeviceDesc%=RICOHCARDBUS, PCI\VEN_1180&DEV_0476
%PCI\VEN_1180&DEV_0478.DeviceDesc%=RICOHCARDBUS, PCI\VEN_1180&DEV_0478
%PCI\VEN_1180&DEV_0475.DeviceDesc%=RICOHCARDBUS, PCI\VEN_1180&DEV_0475

[Trident]
%Trident094.DeviceDesc%=PCIC, PCI\VEN_119B&DEV_1221
%PCI\VEN_1023&DEV_0194.DeviceDesc%=TRIDENTCARDBUS, PCI\VEN_1023&DEV_0194

[O2Micro]
%PCI\VEN_1217&DEV_6729.DeviceDesc%=PCIC, PCI\VEN_1217&DEV_6729
%PCI\VEN_1217&DEV_673a.DeviceDesc%=PCIC, PCI\VEN_1217&DEV_673a
%PCI\VEN_1217&DEV_6832.DeviceDesc%=CARDBUS, PCI\VEN_1217&DEV_6832
%PCI\VEN_1217&DEV_6836.DeviceDesc%=CARDBUS, PCI\VEN_1217&DEV_6836

;
;   Databook install section
;
[DBK0000]
CopyFiles=CSCopyFiles,@dbkvssd.vxd
AddReg=CSReg,DatabookReg
LogConfig=*DBK0000.LC0,*DBK0000.LC1,*DBK0000.LC2,*DBK0000.LC3

[*DBK0000.Det]
AddReg=ForceCopy
LogConfig=*DBK0000.LC0,*DBK0000.LC1,*DBK0000.LC2,*DBK0000.LC3

[*DBK0000.LC0]
ConfigPriority=DESIRED
IOConfig=20@200-3FF%FFE0(3ff::)
IRQConfig=3,4,5,7,10,11,14

[*DBK0000.LC1]
ConfigPriority=DESIRED
IOConfig=10@200-3FF%FFF0(3ff::)
IRQConfig=3,4,5,7,10,11,14

[*DBK0000.LC2]
ConfigPriority=NORMAL
IOConfig=20@200-3FF%FFE0(3ff::)

[*DBK0000.LC3]
ConfigPriority=NORMAL
IOConfig=10@200-3FF%FFF0(3ff::)

[DBK0402]
CopyFiles=CSCopyFiles,@dbkvssd.vxd
AddReg=CSReg,DatabookReg,DBK0402.Reg
LogConfig=*DBK0000.LC0,*DBK0000.LC1,*DBK0000.LC2,*DBK0000.LC3

[DBK0402.Reg]
HKR,Override,0000,1,00,04,00,00,00,00,00,00,20,00,00,00,02,00,00,00,01,00,0c,00,00,00,00,00,00,00,00,00,f0,ff,10,00,00,01,ff,ff,00,00,00,00,10,00,00,00,04,00,00,00,00,00,00,00,fc,cc,00,00,00,00,00,00

[DBK1402]                       ;DB86184
CopyFiles=CSCopyFiles,@dbkvssd.vxd
AddReg=CSReg,DatabookReg
LogConfig=*DBK0000.LC0,*DBK0000.LC1,*DBK0000.LC2,*DBK0000.LC3

[DatabookReg]
HKR,,Driver,,"DbkVssD.vxd"
HKR,,Properties,,"MSPCIC.dll, PCICProperties"

;
;   PCIC or compatible controller
;
[PCIC]
CopyFiles=CSCopyfiles, @socketsv.vxd
AddReg=CSReg, PCICReg
LogConfig=*PNP0E00.LC0,*PNP0E00.LC1,*PNP0E00.LC2,*PNP0E00.LC3,*PNP0E00.LC4,*PNP0E00.LC5

[PCIC.PosDup]
*PNP0E00

[PCICReg]
HKR,,Driver,,"SocketSv.vxd"
HKR,,Properties,,"MSPCIC.dll, PCICProperties"

[*PNP0E00.Det]
AddReg=ForceCopy
LogConfig=*PNP0E00.LC0,*PNP0E00.LC1,*PNP0E00.LC2,*PNP0E00.LC3,*PNP0E00.LC4,*PNP0E00.LC5

[*PNP0E00.LC0]
ConfigPriority=DESIRED
IOConfig=3e0-3e1(3ff::)
IRQConfig=3,4,5,7,9,10,11,14

[*PNP0E00.LC1]
ConfigPriority=NORMAL
IOConfig=3e0-3e1(3ff::)

[*PNP0E00.LC2]
ConfigPriority=DESIRED
IOConfig=3e0-3e1(3ff::)
IOConfig=3e2-3e3(3ff::)
IRQConfig=3,4,5,7,9,10,11,14

[*PNP0E00.LC3]
ConfigPriority=NORMAL
IOConfig=3e0-3e1(3ff::)
IOConfig=3e2-3e3(3ff::)

[*PNP0E00.LC4]
ConfigPriority=HARDRECONFIG
IOConfig=2@100-3FF%FFFE(3ff::)
IRQConfig=3,4,5,7,9,10,11,14

[*PNP0E00.LC5]
ConfigPriority=HARDRECONFIG
IOConfig=2@100-3FF%FFFE(3ff::)

;
;   VLSI ELC controller
;
[VLELC]
CopyFiles=CSCopyfiles, @socketsv.vxd
AddReg=CSReg, PCICReg, VLSIReg
LogConfig=*PNP0E02.LC0,*PNP0E02.LC1,*PNP0E02.LC2,*PNP0E02.LC3

[VLELC.PosDup]
*PNP0E02

[VLSIReg]
HKR,,PCICIRQMap,3,00,00,00,03,04,05,0F,07,00,09,0A,0B,0C,00,0E,00
;HKR,,PCICOptions,3,B8,5E,00,00

[*PNP0E02.Det]
AddReg=ForceCopy
LogConfig=*PNP0E02.LC0,*PNP0E02.LC1,*PNP0E02.LC2,*PNP0E02.LC3

[*PNP0E02.LC0]
ConfigPriority=DESIRED
IOConfig=3e0-3e1(3ff::)
IRQConfig=3,4,5,7,9,10,11,14

[*PNP0E02.LC1]
ConfigPriority=DESIRED
IOConfig=3e0-3e1(3ff::)
IOConfig=3e4-3e5(3ff::)
IRQConfig=3,4,5,7,9,10,11,14

[*PNP0E02.LC2]
ConfigPriority=NORMAL
IOConfig=3e0-3e1(3ff::)

[*PNP0E02.LC3]
ConfigPriority=NORMAL
IOConfig=3e0-3e1(3ff::)
IOConfig=3e4-3e5(3ff::)

;
; Card bus
;
[CARDBUS]
CopyFiles=CSCopyfiles, @cbss.vxd
AddReg=CSReg, CARDBUSReg

[TOPIC]
CopyFiles=CSCopyfiles, @cbss.vxd
AddReg=CSReg, CARDBUSReg, TOPICReg

[TOPICReg]
HKR,,CBSSIRQMap,3,00,00,00,03,04,05,00,07,00,09,0A,0B,0C,00,0E,0F
HKR,,CBSSCSContextRanges,3,3e,00,02,00,44,00,04,00,80,00,14,00,a0,00,08,00,ac,00,02,00

[TICARDBUS]
CopyFiles=CSCopyfiles, @cbss.vxd
AddReg=CSReg, CARDBUSReg, TICBReg

[NTICARDBUS]
CopyFiles=CSCopyfiles, @cbss.vxd
AddReg=CSReg, CARDBUSReg, NEWTIREG

[NEWTIREG]
HKR,,CBSSCompatID, 3, 4c, 10, 15, ac

[TICBReg]
HKR,,CBSSCSContextRanges,3,3e,00,02,00,44,00,04,00,80,00,1c,00

[DBKCARDBUS]
CopyFiles=CSCopyfiles, @cbss.vxd
AddReg=CSReg, CARDBUSReg, DBKCBReg

[DBKCBReg]
HKR,,CBSSCSContextRanges,3,3e,00,02,00,44,00,04,00,80,00,0c,00,a0,00,02,00

[CLCARDBUS]
CopyFiles=CSCopyfiles, @cbss.vxd
AddReg=CSReg, CARDBUSReg, CLCBReg

[CLCBReg]
HKR,,CBSSCSContextRanges,3,3e,00,02,00,44,00,0c,00
HKR,,CBSSEXCAContextRanges,3,02,00,45,00,03,01,01,00,0a,01,02,00,22,01,1a,00

[OPTICARDBUS]
CopyFiles=CSCopyfiles, @cbss.vxd
AddReg=CSReg, CARDBUSReg, OPTICBReg

[OPTICBReg]
HKR,,CBSSCSContextRanges,3,3e,00,02,00,44,00,04,00,50,00,24,00

[RICOHCARDBUS]
CopyFiles=CSCopyfiles, @cbss.vxd
AddReg=CSReg, CARDBUSReg, RICOHCBReg

[RICOHCBReg]
HKR,,CBSSCSContextRanges,3,3e,00,02,00,44,00,04,00,80,00,0c,00,90,00,04,00
HKR,,CBSSCBContextRanges,3,00,00,14,00,20,00,04,00
HKR,,CBSSCompatID,3,80,11,66,04

[TRIDENTCARDBUS]
CopyFiles=CSCopyfiles, @cbss.vxd
AddReg=CSReg, CARDBUSReg, TRIDENTCBReg

[TRIDENTCBReg]
HKR,,CBSSCSContextRanges,3,3e,00,02,00,44,00,04,00,80,00,04,00,90,00,04,00
HKR,,CBSSCBContextRanges,3,00,00,14,00,20,00,04,00

[CARDBUSReg]
HKR,,Driver,,"cbss.vxd"

[CARDBUS.PosDup]
*PNP0E00

[TOPIC.PosDup]
*PNP0E00

;
;   Card services information
;
[CSCopyfiles]
PCCard.vxd
csmapper.sys
carddrv.exe
SRAMMTD.VXD
FLS1MTD.VXD
FLS2MTD.VXD

[CSReg]
HKR,,DevLoader,,"PCCARD.vxd"
HKLM,Software\Microsoft\Windows\CurrentVersion\Run,SystemTray,,"SysTray.Exe"

;
;   Socket Services information
;

;
;   Information about where the files are
;
[DestinationDirs]
DefaultDestDir=11               ; LDID_SYS


[ForceCopy]
HKR,,NoSetupUI,,1

;
;   Config.Sys drivers to remove
;
[ConfigSysDrivers]
;
; Databook
;
CARDSOCK.SYS
CTALKCS.EXE
CARDTALK.SYS
ARIMATN.SYS
CARDTALK.EXE

;
; SystemSoft
;
SS365SL.EXE
SS365SLB.EXE
CS.EXE
SSDBOOK.EXE
SSCIRRUS.EXE
SSVLSI.EXE
CIC.EXE
MS-FLASH.SYS
RALLOC.EXE
SCARD29.EXE
SRAMDRV.EXE
S_IDE.EXE
CARDID.EXE
ATAINIT.EXE
ATADRV.EXE
CSALLOC.EXE
CARDINFO.EXE
SS365LP.EXE
SSVADEM.EXE
SSIBM720.EXE
MTDDRV.EXE
MTSRAM.EXE
CARD_BAP.EXE
PCIC.EXE
MEMDRV.EXE
DBLFLASH.EXE
SS6941.EXE
SS6942.EXE
SSPPEC.EXE
MTAA.EXE
MTAB.EXE
MTI1.EXE
MTI2P.EXE
MTAMP.EXE
SSMSFLSH.EXE
FTL.EXE
CS_APM.EXE
CARDLITE.EXE
SSTPIC95.EXE

;
; Phoenix/Toshiba
;
CACCESS.SYS
PCMP615B.EXE
PCMCS.EXE
PCMMTD.EXE
PCMATA.SYS
PCMATADD.SYS
PCMSCD.EXE
PCMFDD.EXE
PCMFFCS.EXE
PCMSS.EXE
CNFIGNAM.EXE
PCM.EXE
PCMRMAN.EXE
PCMRMAN.SYS
PCMSSCL.EXE
PCMSSDB.EXE
PCMSSIT.EXE
PCMSSRC.EXE
PCMSSVD.EXE
PCMWARN.EXE
PCMCS95.EXE

;
; Award
;
PCSS.EXE
SSPCIC.EXE
SSPHIC.EXE
SSTACT.EXE
SSTCIC.EXE
SSTPP163.EXE
PCCS.EXE
PCRM.EXE
PCENABLE.EXE
PCDISK.EXE
PCPREP.EXE
PCCARD.EXE
SS82086.SYS
PCDIRTY.EXE
DOSCARD.EXE
TOPIC.SYS

;
; Compaq
;
PCMSMIX.EXE

;
; IBM
;
IBMDOSCS.SYS
PCMCIA.SYS
IBMDSS01.SYS
IBM2SS01.SYS
DICRMU01.SYS
ICRMU01.SYS
$ICPMDOS.SYS
$ICPMOS2.SYS
PCMCIAON.EXE
PCMCIAOF.EXE
EZPLAY.EXE
EZPLAYW.EXE
AUTODRV.SYS
AUTODRV2.SYS
SRAMDRV2.SYS
DISKDRV.SYS
IBM2SS02.SYS
IBM2SS03.SYS
IBMDSS02.SYS
IBMDSS03.SYS
SS2PCIC1.SYS
SSDPCIC1.SYS
SS2TCIC1.SYS
SSDTCIC1.SYS
VPCMCIA.SYS
IBMDOSCS.SYS
IBMDSCSE.SYS
RMUDOSAT.SYS
PCM2FLSH.SYS
PAWATA.SYS
PAWATAS.SYS
PAWATASF.SYS
FLSH2MTD.SYS
PCMSSDIF.SYS
FLSHDMTD.SYS
EZLAUNCH.EXE


;
; TDK
;
TDKMODEM.EXE
MODINSTL.EXE
MODACTIV.EXE
SET3300.COM
TDKCARD.EXE
SSDOS.COM

;
; HP
;
OBSS.EXE

;
; Enablers
;
ENABLEEA.EXE
SKTNDIS.EXE
MA460.SYS
cendis.exe
b8895.com
modem.exe
PCMSM.COM
ETHERNET.SYS
POINTETH.SYS
TOSHETH.SYS
PCMDMCS.COM
PCMNICCS.DOS
CONXDRV.EXE
PMODEM.SYS
PCMCIA1.SYS
PCMCIA2.SYS
SETPCMC.EXE
PCMCIA.EXE
S-PCMCIA.EXE
T-PCMCIA.EXE
MSETUP.EXE
PRR.EXE
MODCFG.EXE
ADAPTER.EXE
SS365SL.EXE
SSDBOOK.EXE
CS.EXE
CSALLOC.EXE
PCMDM.COM
ECCTEST.EXE
POINTETH.SYS
TOSHETH.SYS
SHARPETH.SYS
PCMDM.DOS
NICESS.COM
VMISS.SYS
FJTMAC.DOS
PSETUP.EXE
POINTETH.SYS
TOSHTR.SYS
TOKENRNG.SYS
POINTTR.SYS
PDLTOK.DOS
PCMDMCS.COM
PCMNICCS.DOS
SETMHZ.EXE
NMCMSSND.SYS
SWAPBOX.SYS
1130_XX.SYS

;
;   Autoexec.Bat drivers to remove
;
[AutoexecBatDrivers]
ENABLEEA
SKTNDIS
SETMHZ
CS_APM
CECFG
OBSS
WJSSENAB
CEMCFG
CE2CFG
CXCFG
CFG2INI

;
;   System.Ini drivers to remove
;
[SystemIniDrivers]
;
; compaq
;
cs.386
cpqevent.386
ssvrdd.386
ssvcd311.386
pccard.386
pccardrm.386

;
; Phoenix
;
PCMVCD.386

;
; SystemSoft
;
cs_pmc.386
vpmc.386
NMCMSSND.386

;
;   System.Ini drivers= DLLs to remove
;
[SystemIniDriversLine]
sswincs.dll
nmcmssnd.drv

;
; SystemSoft
;
cardpwrd.drv
pmc.drv


;
;   Win.Ini run= EXEs to remove
;
[WinIniRunLine]
cpqevent
pccard
cardview

[Strings]
ClassName="PCMCIA socket"
MS="Microsoft"

;
;   Manufacturer name strings
;
GenDrvs="(Standard PCMCIA drivers)"
IntelMfg="Intel"
DatabookMfg="Databook"
VLSIMfg="VLSI"
CompaqMfg="Compaq"
CirrusMfg="Cirrus Logic"
VademMfg="Vadem"
MXTR="Maxtor"
SCM="SCM SwapBox"
Toshiba="Toshiba"
TI="Texas Instruments"
OPTi="OPTi"
Ricoh="RICOH"
Trident="Trident"
IBMMfg="IBM"
O2MicroMfg="O2Micro/ROHM"
SMC="SMC"

;
;   Device Decription strings
;
PCCard.DeviceDesc="PCMCIA Card Services"
GenPCIC="PCIC or compatible PCMCIA controller"
IntelProto="Intel PCIC compatible PCMCIA controller"
Cirrus.DeviceDesc="Cirrus Logic PCIC compatible PCMCIA controller"
PCI\VEN_1013&DEV_1100.DeviceDesc="Cirrus Logic PCIC compatible PCI to PCMCIA Bridge"
Vadem.DeviceDesc="Vadem PCIC compatible PCMCIA controller"
*VDM0469.DeviceDesc="Vadem PCIC compatible Plug and Play PCMCIA controller"
SCM.DeviceDesc="SCM SwapBox Family PCMCIA controller"
*SCM0469.DeviceDesc="SCM SwapBox Family Plug and Play PCMCIA controller"

;
;   Strings with "*PNPxxxx" are descriptions used by hardware detection
;   for PCMCIA controllers
;
*PNP0E00.DeviceDesc="PCIC Compatible PCMCIA Controller"
*PNP0E02.DeviceDesc="VLSI PCIC Compatible PCMCIA Controller with ELC Extensions"
*IBM0030.DeviceDesc="IBM King ISA Plug and Play PCMCIA Controller"
*DBK0000.DeviceDesc="Databook ISA PCMCIA Controller"
*DBK0402.DeviceDesc="Databook Plug and Play PCMCIA Controller based on DB86084"
*DBK0204.DeviceDesc="Databook Plug and Play PCMCIA Controller based on DB86084"
*DBK1402.DeviceDesc="Databook Plug and Play PCMCIA Controller based on DB86184"
*DBK0214.DeviceDesc="Databook Plug and Play PCMCIA Controller based on DB86184"
PCI\VEN_10B3&DEV_3106.DeviceDesc="Databook DB87144 CardBus Controller"
PCI\VEN_10B8&DEV_B106.DeviceDesc="SMC34C90 CardBus Controller"
MXTR.Deskrunner="MobileMax Deskrunner ISA PCMCIA Controller"
*CPQA0DE.DeviceDesc="Compaq PCMCIA Controller"
PCI\VEN_8086&DEV_1221.DeviceDesc="Intel 82092AA PCI to PCMCIA Bridge"
IntelPCI="Intel PCI to PCMCIA Bridge"
PCI\CC_0607.DeviceDesc="Generic CardBus Controller"
PCI\VEN_1179&DEV_060A.DeviceDesc="Toshiba ToPIC95 CardBus Controller"
PCI\VEN_1179&DEV_060F.DeviceDesc="Toshiba ToPIC97 CardBus Controller"
PCI\VEN_104C&DEV_AC12.DeviceDesc="Texas Instruments PCI-1130 CardBus Controller"
PCI\VEN_104C&DEV_AC13.DeviceDesc="Texas Instruments PCI-1031 PCMCIA Controller"
PCI\VEN_104C&DEV_AC15.DeviceDesc="Texas Instruments PCI-1131 CardBus Controller"
PCI\VEN_104C&DEV_AC16.DeviceDesc="Texas Instruments PCI-1250 CardBus Controller"
PCI\VEN_104C&DEV_AC17.DeviceDesc="Texas Instruments PCI-1220 CardBus Controller"
PCI\VEN_104C&DEV_AC18.DeviceDesc="Texas Instruments PCI-1260 CardBus Controller"
PCI\VEN_104C&DEV_AC19.DeviceDesc="Texas Instruments PCI-1221 CardBus Controller"
PCI\VEN_104C&DEV_AC1A.DeviceDesc="Texas Instruments PCI-1210 CardBus Controller"
PCI\VEN_104C&DEV_AC1B.DeviceDesc="Texas Instruments PCI-1450 CardBus Controller"
PCI\VEN_104C&DEV_AC1C.DeviceDesc="Texas Instruments PCI-1225 CardBus Controller"
PCI\VEN_104C&DEV_AC1D.DeviceDesc="Texas Instruments PCI-1251 CardBus Controller"
PCI\VEN_1045&DEV_C824.DeviceDesc="OPTi 82C824 CardBus Controller"
PCI\VEN_1045&DEV_C814.DeviceDesc="OPTi 82C814 Docking Controller"
PCI\VEN_1013&DEV_1110.DeviceDesc="Cirrus Logic PD6832 CardBus Controller"
PCI\VEN_1013&DEV_1112.DeviceDesc="Cirrus Logic PD6834 CardBus Controller"
PCI\VEN_1013&DEV_1113.DeviceDesc="Cirrus Logic PD6833 CardBus Controller"
PCI\VEN_1180&DEV_0466.DeviceDesc="Ricoh RL5C466 CardBus Controller"
PCI\VEN_1180&DEV_0465.DeviceDesc="Ricoh RL5C465 CardBus Controller"
PCI\VEN_1180&DEV_0476.DeviceDesc="Ricoh RL5C476 CardBus Controller"
PCI\VEN_1180&DEV_0478.DeviceDesc="Ricoh RL5C478 CardBus Controller"
PCI\VEN_1180&DEV_0475.DeviceDesc="Ricoh RL5C475 CardBus Controller"
Trident094.DeviceDesc="Trident Omega-82C094 PCI to PCMCIA Bridge"
PCI\VEN_1023&DEV_0194.DeviceDesc="Trident 82C194 CardBus Controller"
PCI\VEN_1217&DEV_6729.DeviceDesc="O2 Micro OZ6729 PCI to PCMCIA Bridge"
PCI\VEN_1217&DEV_673a.DeviceDesc="O2 Micro OZ6730 PCI to PCMCIA Bridge"
PCI\VEN_1217&DEV_6832.DeviceDesc="O2 Micro OZ6832/6833 CardBus Controller"
PCI\VEN_1217&DEV_6836.DeviceDesc="O2 Micro/ROHM OZ6836/6860 CardBus Controller"

