Xircom Ethernet 10/100+Modem 56 - Result Codes

#

Table of Contents | Previous Page | Next Page

# Ethernet 10/100+Modem 56
Modem Result Codes

The following list details modem result codes that appear after the executing of a modem AT command.

### Modem Result Codes

Long | Short | Description
OK | 0 | Command successfully executed
CONNECT | 1 | Modem connected to line
RING | 2 | Incoming ring signal detected
NO CARRIER | 3 | Carrier detect failed/carrier dropped
ERROR | 4 | Command is invalid
NO DIALTONE | 6 | No tone during interval set with S6
BUSY | 7 | Busy signal detected
NO ANSWER | 8 | Remote end never answered
CONNECT 2400 EC* | 10 | Connection at 2400 bit/s
CONNECT 4800 EC* | 11 | Connection at 4800 bit/s
CONNECT 9600 EC* | 12 | Connection at 9600 bit/s
CONNECT 14400 EC* | 13 | Connection at 14400 bit/s
CONNECT 19200 EC* | 14 | Connection at 19200 bit/s
CONNECT 7200 EC* | 24 | Connection at 7200 bit/s
CONNECT 12000 EC* | 25 | Connection at 12000 bit/s
CONNECT 16800 EC* | 86 | Connection at 16800 bit/s
CONNECT 300 EC* | 40 | Connection at 300 bit/s
CONNECT 21600 EC* | 55 | Connection at 21600 bit/s
CONNECT 24000 EC* | 56 | Connection at 24000 bit/s
CONNECT 26400 EC* | 57 | Connection at 26400 bit/s
CONNECT 28800 EC* | 58 | Connection at 28800 bit/s
CONNECT 31200 EC* | 59 | Connection at 31200 bit/s
CONNECT 33600 EC* | 60 | Connection at 33600 bit/s
CONNECT 38400 EC* | 28 | Connection at 38400 bit/s (DTE rate)
CONNECT 57600 EC* | 18 | Connection at 57600 bit/s (DTE rate)
CONNECT 115200 EC* | 87 | Connection at 115200 bit/s (DTE rate)
DELAYED | 88 | Delay in effect for dialed number
BLACKLISTED | 89 | Dialed number is blacklisted
BLACKLIST FULL | 90 | Blacklist is full
CONNECT 32000 EC* | 70 | Connection at 32000 bit/s (K56flex mode) or V.90
CONNECT 34000 EC* | 71 | Connection at 34000 bit/s (K56flex mode)
CONNECT 36000 EC* | 72 | Connection at 36000 bit/s (K56flex mode) or V.90
CONNECT 38000 EC* | 73 | Connection at 38000 bit/s (K56flex mode)
CONNECT 40000 EC* | 74 | Connection at 40000 bit/s (K56flex mode) or V.90
CONNECT 42000 EC* | 75 | Connection at 42000 bit/s (K56flex mode)
CONNECT 44000 EC* | 76 | Connection at 44000 bit/s (K56flex mode) or V.90
CONNECT 46000 EC* | 77 | Connection at 46000 bit/s (K56flex mode)
CONNECT 48000 EC* | 78 | Connection at 48000 bit/s (K56flex mode) or V.90
CONNECT 50000 EC* | 79 | Connection at 50000 bit/s (K56flex mode)
CONNECT 52000 EC* | 80 | Connection at 52000 bit/s (K56flex mode) or V.90
CONNECT 54000 EC* | 81 | Connection at 54000 bit/s (K56flex mode)
CONNECT 56000 EC* | 82 | Connection at 56000 bit/s (K56flex mode)
CONNECT 28000 EC* | 100 | Connection at 28000 bit/s (V.90 mode)
CONNECT 29333 EC* | 101 | Connection at 29333 bit/s (V.90 mode)
CONNECT 30666 EC* | 102 | Connection at 30666 bit/s (V.90 mode)
CONNECT 33333 EC* | 103 | Connection at 33333 bit/s (V.90 mode)
CONNECT 34666 EC* | 104 | Connection at 34666 bit/s (V.90 mode)
CONNECT 37333 EC* | 105 | Connection at 37333 bit/s (V.90 mode)
CONNECT 38666 EC* | 106 | Connection at 38666 bit/s (V.90 mode)
CONNECT 41333 EC* | 107 | Connection at 41333 bit/s (V.90 mode)
CONNECT 42666 EC* | 108 | Connection at 42666 bit/s (V.90 mode)
CONNECT 45333 EC* | 109 | Connection at 45333 bit/s (V.90 mode)
CONNECT 46666 EC* | 110 | Connection at 46666 bit/s (V.90 mode)
CONNECT 49333 EC* | 111 | Connection at 49333 bit/s (V.90 mode)
CONNECT 50666 EC* | 112 | Connection at 50666 bit/s (V.90 mode)
CONNECT 53333 EC* | 113 | Connection at 53333 bit/s (V.90 mode)
CONNECT 54666 EC* | 114 | Connection at 54666 bit/s (V.90 mode)

* EC only appears when the extended result codes configuration option is enabled. EC is replaced by one of the following symbols, depending on the error control method used:
V42bis - V.42 error control and V.42bis data compression.
V42 - V.42 error control only.
MNP5 - MNP class 4 error control and MNP class 5 data compression.
MNP 4 - MNP class 4 error control only.
NoEC - No error control protocol.

Table of Contents | Previous Page | Next Page