[data]
type=network
version="3.11.136"

[disks]
1=., "Xircom Ethernet 10/100 + Modem 56 Network Driver Disk", disk 1

[netcard]
XIRCMAC="Xircom XCEM NDIS 2.01 Real Mode", 0, NDIS, Ethernet, REAL, XIRCMAC_INST, XIRCMAC_INI
XIRC$ODI="Xircom XCEM ODI for Netware", 0, NDIS, Ethernet, 0x04, XIRCODI_INST, XIRCODI_INI

[XIRCODI_INST]
mlid=xcemodi.com

[XIRCODI_INI]

[XIRCMAC_INST]
netdir=1:xcemndis.exe
device=xcemndis.exe, @netdir\xcemndis.exe
mlid=1:xcemodi.com

[XIRCMAC_INI]
DriverName=XIRCOM$
param=INT,"INTERRUPT",int,"3,15,1",5,0x02
param=LINESPEED,"Linespeed",enum,"100 Mbps,100,10 Mbps ,10",100,0x02
param=IOADDRESS,"IOADDRESS",hex,"0x200,0x380,0x20",0x320,0x02
param=MEM,"MEMORY",hex,"0xC0000,0xE8000,0x02000",0xD2000,0x02
param=MODE,"MODE",text,"MEMORY,IO","MEMORY",0x02
param=LINKDISABLE,"Link Disable",keyonly,,,0x02
param=LINEMODE,"Force Line Mode",enum,"Half duplex,HALF,Full Duplex,FULL",HALF,0x02
param=NOEARLYTX,"No Early Transmit",keyonly,,,0x02
param=COM1,"COM1",keyonly,,,0x02
param=COM2,"COM2",keyonly,,,0x02
param=COM3,"COM3",keyonly,,,0x02
param=COM4,"COM4",keyonly,,,0x02



