[ID]
Name=Class73
Type=10

[LoadValues]
DialStr=0123456789,!()-*#
ToneStr=T
PulseStr=P
ICDelay=5
DelayValue=500

[Commands]
Setup=AT&FS95=1W2^M
Restore=AT&F^M
DialPrfx=ATD
DialSufx=^M
Disc=ATH^M
Esc=~~~+++~~~
Reset=ATZ^M

[ResultCodes]
NCBUSY=BUSY
NCVOICE=VOICE
NCTIMEOUT=TIMEOUT
NCDIALTONE=NO DIAL
NCCARRIER=NO CARRIER
NCANSWER=NO ANSWER
C300=CONNECT^M
C1200=CONNECT 1200
C2400=CONNECT 2400
C4800=CONNECT 4800
C7200=CONNECT 7200
C9600=CONNECT 9600
C12000=CONNECT 12000
C14400=CONNECT 14400
C16800=CONNECT 16800
C19200=CONNECT 19200
C21600=CONNECT 21600
C24000=CONNECT 24000
C26400=CONNECT 26400
C28800=CONNECT 28800
C29333=CONNECT 29333
C30666=CONNECT 30666
C31200=CONNECT 31200
C32000=CONNECT 32000
C33333=CONNECT 33333
C33600=CONNECT 33600
C34000=CONNECT 34000
C34666=CONNECT 34666
C36000=CONNECT 36000
C37333=CONNECT 37333
C38000=CONNECT 38000
C38400=CONNECT 38400
C38666=CARRIER 38666
C40000=CONNECT 40000
C41333=CONNECT 41333
C42000=CONNECT 42000
C42666=CONNECT 42666
C44000=CONNECT 44000
C45333=CONNECT 45333
C46000=CONNECT 46000
C46666=CONNECT 46666
C48000=CONNECT 48000
C49333=CONNECT 49333
C50000=CONNECT 50000
C50666=CONNECT 50666
C52000=CONNECT 52000
C53333=CONNECT 53333
C54000=CONNECT 54000
C54666=CONNECT 54666
C56000=CONNECT 56000
C57600=CONNECT 57600

CmdOK=OK^M
CmdErr=ERROR^M
CmdEsc=+++




